|  |  |  |  |
| --- | --- | --- | --- |
|  | United Nations | ECE/TRANS/WP.29/GRPE/2017/3 | |
| Description: _unlogo | **Economic and Social Council** | | Distr.: General  25 October 2016  Original: English |

**Economic Commission for Europe**

Inland Transport Committee

**World Forum for Harmonization of Vehicle Regulations**

**Working Party on Pollution and Energy**

**Seventy-fourth session**

Geneva, 10-13 January 2017

Item 3(b) of the provisional agenda

**Light vehicles – Global Technical**

**Regulation No. 15 on Worldwide harmonized**

**Light vehicles Test Procedure (WLTP)**

**Proposal for a new global technical regulation on Evaporative emission test procedure for the Worldwide harmonized Light vehicles Test Procedure (WLTP EVAP)**

**Submitted by the Informal Working Group on Worldwide harmonized Light vehicles Test Procedure (WLTP)**[[1]](#footnote-2)\*

The text reproduced below was prepared by the Evaporative Task Force of the Informal Working Group (IWG) on Worldwide harmonized Light vehicles Test Procedure (WLTP) in line with Phase 2 of its mandate (ECE/TRANS/WP.29/AC.3/44). The IWG on WLTP referred to a first draft of this proposal (GRPE-73-12) at the seventy-third session of GRPE (see report ECE/TRANS/WP.29/GRPE/73, para. 12).

Draft global technical regulation on Evaporative emission test procedure for the Worldwide harmonized Light vehicle Test Procedure (WLTP EVAP)

I. Statement of technical rationale and justification

A. Introduction

1. The compliance with emission standards is a central issue of vehicle certification worldwide. Emissions comprise criteria pollutants having a direct (mainly local) negative impact on health and environment, as well as pollutants having a negative environmental impact on a global scale. Regulatory emission standards typically are complex documents, describing measurement procedures under a variety of well-defined conditions, setting limit values for emissions, but also defining other elements such as the durability and on-board monitoring of emission control devices.

2. Most manufacturers produce vehicles for a global clientele or at least for several regions. Albeit vehicles are not identical worldwide since vehicle types and models tend to cater to local tastes and living conditions, the compliance with different emission standards in each region creates high burdens from an administrative and vehicle design point of view. Vehicle manufacturers, therefore, have a strong interest in harmonizing vehicle emission test procedures and performance requirements as much as possible on a global scale. Regulators also have an interest in global harmonization since it offers more efficient development and adaptation to technical progress, potential collaboration at market surveillance and facilitates the exchange of information between authorities.

3. As a consequence stakeholders launched the work on the Worldwide harmonized Light vehicle Test Procedure (WLTP) which aims at harmonizing emission-related test procedures for light duty vehicles to the extent this is possible. One of the aspects covered within the mandate for WLTP is the evaporative emission test procedure.

4. Evaporative emissions from vehicles is a complex phenomenon which depends on multiple factors, that ranges from climate conditions to fuel properties, from driving and parking patterns to the technology used to control these emissions.

5. Evaporative emissions from a vehicle can be defined, in a very generic way, as Volatile Organic Compounds (VOCs) emitted by the vehicle itself in different operating conditions but not directly derived from the combustion process. In petrol vehicles the most important potential source of evaporative emissions is the loss of fuel through the evaporation and permeation mechanisms from the fuel storing system. Fuel-related evaporative emissions may occur during any vehicle operation including parking events, normal driving and vehicle refuelling.

6. VOCs may also be emitted by specific components of the vehicle such as tyres, interior trim, plastics or by other fluids (e.g. windshield washer fluid). These non-fuel related emissions are usually quite low, not dependent on how the vehicle is used or on the quality of the fuel, and tend to decrease over time. Evaporative emissions in general do not represent a significant problem for diesel vehicles due to the very low vapour pressure of diesel fuel.

7. During parking events, an increase of the temperature of the fuel in the tank due to rising ambient temperature and solar radiation may lead to evaporation of the lightest petrol fractions with a corresponding increase of the pressure inside the tank. The fuel tank, by design, is usually vented to the atmosphere through a pressure relief valve, so that the tank pressure is maintained slightly above atmospheric pressure. If the pressure inside the tank rises above that value, a mixture of air and petrol vapours may be released into the atmosphere. In modern vehicles the tank is vented through an activated carbon canister which adsorbs and stores the hydrocarbons (HC) preventing emissions to the atmosphere. This carbon canister has a limited adsorbing capacity (depending on several factors of which the most important are the carbon quality and mass as well as the temperature) and has to be periodically purged to desorb the stored hydrocarbons. This occurs during vehicle driving since part of the combustion air flows through the canister removing the adsorbed hydrocarbons which are then burned inside the engine.

The use of sealed tanks may represent an alternative solution to the system described above especially for hybrid vehicles. Due to the potentially reduced time of operation of the combustion engine in hybrids and plug-in hybrids, proper purging the carbon canister may represent an issue. As a consequence the carbon canister may not have enough capacity to store fuel vapours during a parking event. A sealed tank is by design a closed system that can store fuel vapours inside the tank at least up to a certain maximum pressure. If this maximum pressure is not reached, a sealed tank has the capability to reduce breathing losses basically to zero. However, in general the sealed tank needs to be depressurised before refuelling to ensure safe operation. Depressurisation is generally achieved through a pressure relief valve operated by the customer. Obviously the mixture of air and vapours released through the pressure relief valve should not be vented directly to the atmosphere in order to avoid reducing significantly the benefits of this technology. This is usually achieved by releasing the pressure through a carbon canister which is then purged when the combustion engine runs.

In severe temperature conditions the pressure inside the tank might exceed the maximum value allowed by the design and the material of the tank. This maximum value is the result of a compromise between the performance requirements and the cost/weight of the tank. The latter aspect is particularly important for the impact on fuel consumption. For this reason a pressure relief valve is an essential safety feature which will avoid the risk of rupturing the tank.

The pressure increase inside the tank with rising temperature may be reduce by insulating the tank itself. This means that the temperature of the fuel will remain always something lower than the ambient temperature. This aspect has been taken into account when designing the test procedure.

8. In normal vehicle driving conditions, in addition to the ambient air and solar radiation, the temperature of the fuel in the tank may increase as a consequence of the heat coming from other sources (hot engine and exhaust system, fuel pump, fuel return if present, road surface that may be significantly hotter than the ambient air). The balance among the fuel evaporation rate, the amount of fuel being pumped to the engine and the purge flow rate through the canister will determine the carbon canister loading which could lead to excessive emissions in case of breakthrough/saturation. These emissions are known as running losses.

9. Hydrocarbons also escapes the vehicle’s fuel system by permeation through the plastic and rubber components; e.g., hoses, seals, and in vehicles with a non-metallic tank, the fuel tank itself. Permeation does not occur through an opening; instead individual fuel molecules penetrate (i.e. they effectively mix with) the walls of the various components and eventually find their way to the outside. Fuel permeation is significant mainly for plastic or elastomeric materials, depends strongly from the temperature and usually occurs in any vehicle operating conditions.

10. Another important source of evaporative emissions is the refuelling operation. When liquid fuel is delivered into the tank the air/petrol vapour mixture present in the tank is displaced and may be released into the atmosphere. Refuelling emissions are partially controlled through the maximum allowed fuel vapour pressure by reducing its value during the hot season. In addition, evaporative emissions during the refuelling operation can be controlled in two different ways. One method is the so-called "Stage II" vapour recovery system. The fuel nozzle is designed to draw the air/petrol vapour mixture displaced by the liquid fuel entering the tank and route it to the underground petrol storage tank of the service station. An alternative method is an "On-board Vapour Recovery System" (ORVR), which forces the displaced vapours to be routed to the carbon canister instead of escaping from the refuelling port.

11. An unintended source of HC emissions may occur from leaks in the system. Leaks may occur in the vapour and/or the liquid system as a result of deterioration and/or faulty operations. Examples of deterioration are corrosion of metallic components (e.g. fuel lines, tanks), cracking of rubber hoses, hardening of seals, mechanical failures. On-board diagnostic systems have been developed to check the integrity of the fuel system and are required in some regions.

12. In the existing regional type approval procedures, the various situations that can lead to significant evaporative emissions have been addressed either by developing different tests or by adopting different measures. As an example, in certain regions refuelling emissions are controlled by mandating the use of the Stage II vapour recovery system while in other regions the ORVR approach has been chosen.

13. The need to represent real driving conditions as much as possible to make the performance of vehicles at certification and in real life comparable puts therefore some limitations on the level of harmonization to be achieved since, for instance, ambient temperatures vary widely on a global scale while other potential sources of evaporative emissions are addressed in different ways across the regions (e.g. refuelling emissions or potential leaks).

14. At this time, the WLTP EVAP test procedure focuses only on the evaporative emissions that can occur during parking events. Running losses and refuelling emissions are out of the scope of the current WLTP EVAP procedure.

15. The purpose of a UN global technical regulation (gtr) is its implementation into regional legislation by as many Contracting Parties as possible. However, the scope of regional legislations in terms of vehicle categories concerned depends on regional conditions and cannot be predicted for the time being. On the other hand, according to the rules of the 1998 Agreement, Contracting Parties implementing a gtr must include all equipment falling into the formal gtr scope. Care must be taken so that an unduly large formal scope of the gtr does not prevent its regional implementation. Therefore the formal scope of this gtr is kept mainly for light duty vehicles. However, this limitation of the formal gtr scope does not indicate that it could not be applied to a larger group of vehicle categories by regional legislation. In fact, Contracting Parties are encouraged to extend the scope of regional implementations of this gtr if this is technically, economically and administratively appropriate.

B. Procedural background and future development of the WLTP EVAP

16. In its November 2007 session, the World Forum for Harmonization of Vehicle Regulations (WP.29) decided to set up an Informal Working Group (IWG) under the Working Party on Pollution and Energy (GRPE) to prepare a road map for the development of WLTP. After various meetings and intense discussions, WLTP presented in June 2009 a first road map consisting of three phases, which was subsequently revised a number of times and contains the following main tasks:

(a) Phase 1 (2009–2014): Development of the worldwide harmonized light duty driving cycle and associated test procedure for the common measurement of criteria compounds, CO2, fuel and energy consumption;

(b) Phase 2 (2014–2018): Low temperature/high altitude test procedure, durability, in-service conformity, technical requirements for On-Board Diagnostics (OBD), Mobile Air-Conditioning (MAC) system energy efficiency, off-cycle/real driving emissions, and evaporative emission;

(c) Phase 3 (2018-…): Emission limit values and OBD threshold limits, definition of reference fuels, comparison with regional requirements.

17. It should be noted that since the beginning of the WLTP process, the European Union had a strong political objective set by its own legislation (Regulations (EC) 715/2007 and 692/2008) to review the test procedure for evaporative emissions to ensure that these are effectively limited throughout the normal life of the vehicles under normal conditions of use.

18. The IWG on WLTP presented at the GRPE January 2016 session an updated road map for the Phase 2 including a proposal for the development of the WLTP test procedure for evaporative emissions. A strong desire of the Contracting Parties to develop the gtr by January 2017 was announced.

19. The WLTP EVAP Task Force started its work in February 2016 with the first meeting and ended its work for the development of this gtr in September 2016 with the submission of the current text.

C. Background on test procedures

20. For the development of the WLTP EVAP test procedure, the EVAP Task Force took into account existing legislation as well as the recent review and revision of the European evaporative emission test procedure.

21. The WLTP evaporative emission test procedure focuses only on evaporative emissions that can occur during parking events from both conventional petrol vehicles and hybrid vehicles combining an electric motor with a petrol-fuelled engine.

22. The WLTP evaporative emission test procedure is designed to measure evaporative emissions from a parked vehicle using a sealed housing for evaporative emissions determination (SHED). Two specific situations are considered:

(a) Evaporative emissions occurring immediately after the end of a trip due to residual fuel tank heating and the high temperatures of the engine and fuel system (hot soak test);

(b) Evaporative emissions occurring during a simulated extended parking event (48 hours) while the vehicle is exposed to temperature fluctuations according to a specific profile. This is intended to represent the temperature profile of a hot day (diurnal test). The result of the diurnal test is represented by the total amount of VOCs released in the SHED over a 48 hour period.

For sealed tanks, two other situations are addressed by the WLTP evaporative emission test procedure:

(c) Evaporative emissions that may occur if there is the need to depressurise the tank before refuelling to ensure a safe operation. In order to reduce the pressure inside the tank the air/fuel vapours mixture can be vented to the air through a carbon canister. This operation should also avoid excessive evaporative emissions through the filler neck when the fuel cap/fuel lid is opened. This latter aspect requires that inside the tank there is very limited overpressure compared to the ambient pressure when the fuel cap (or any alternative system used to close the filler neck) is opened.

(d) Evaporative emissions occurring when the maximum tank pressure is reached and the pressure relief valve opens to avoid dangerous situation. In these conditions the emissions could be uncontrolled in case of a fully saturated canister. The test procedure has been designed in order reduce the frequency of this possibility or, alternatively, to control these emissions by means of the carbon canister.

23. The performance of the evaporative emission control system strongly depends on the initial condition of the carbon canister which is expected to adsorb the vapours generated in the tank. In order to simulate realistic conditions, prior to the starting of the hot soak and diurnal tests, the carbon canister is loaded to the breakthrough and then purged by driving the vehicle over a specific combination of WLTC sections (conditioning drive). The conditioning drive cycle was extensively assessed and discussed also on the basis of real world activity data to take into account that the most critical conditions are represented by short trips in urban areas. For this reason, the conditioning drive for Class 2 and 3 vehicles includes one low speed section, two medium speed sections and one high speed section. The extra-high section was excluded. The conditioning drive for Class 1 vehicles includes four low speed sections, two medium speed sections.

24. The test procedure includes also specific provisions to take into account the potential deterioration of the evaporative emission control system efficiency especially in the presence of ethanol in the fuel. The evaporative emission test is carried out with a carbon canister aged both mechanically and chemically according to a specific procedure. In addition, a permeation factor is used to take into account the potential increase over time of the full permeation rate through the tank walls.

25. As far as the fuel is concerned, its vapour pressure and composition (especially ethanol content) have a large effect on evaporative emissions and need therefore to be clearly specified. However, due to regional differences in the market specifications of fuels and in the measurement methods of their relevant properties, regionally different reference fuels need to be recognised. Contracting Parties may select their reference fuels either according to Annex 3 to gtr No. 15 or according to Annex 2 of this gtr.

D. Technical feasibility, anticipated costs and benefits

26. In designing and validating the WLTP EVAP procedure, strong emphasis has been put on its practicability, which is ensured by a number of measures explained above.

27. In general, the WLTP EVAP test procedure has been defined taking into account the technology available for evaporative emission control as well as the existing test facilities.

28. The best available technology performance significantly exceeds the stricter requirements on evaporative emissions which will be introduced in some regions as a results of the adoption of the WLTP EVAP procedure. In general, compared to the technology needed to comply with the requirements based on the 24 hour diurnal test still in force in many regions, the additional cost per vehicle is considered quite limited and eventually compensated by the emission reduction and the fuel savings.

29. Performing a test according to the WLTP EVAP test procedure and complying with the emission limits should not represent a major issue in most cases. Since in many regions the current evaporative test procedure is based on the 24-hour diurnal test, limited upgrades to existing SHEDs might be required to run the 48-hour diurnal test. In other cases, additional SHEDs might be necessary to take into account the longer time needed to complete an evaporative emission tests. Nevertheless, 48-hour diurnal tests are already being performed by most of the car manufacturers since 48-hour and 72-hour diurnal test are already requested for some markets.

30. For a more accurate assessment, costs and benefits would have to be quantified on a regional level since they largely depend on the local conditions (climate, fleet composition, fuel quality, …).

31. As pointed out in the technical rationale and justification, the principle of a globally harmonized light duty vehicle test procedure offers potential cost reductions for vehicle manufacturers. The design of vehicles can be better unified on a global scale and administrative procedures may be simplified. The monetary quantification of these benefits depends largely on the extent and timing of implementations of the WLTP in regional legislation.

II. Text of the global technical regulation

1. Purpose

This global technical regulation (gtr) aims at providing a worldwide harmonized method to determine the levels of evaporative emission from light-duty vehicles in a repeatable and reproducible manner designed to be representative of real world vehicle operation. The results will provide the basis for the regulation of these vehicles within regional type approval and certification procedures.

2. Scope and application

This gtr applies to vehicles of categories 1-2 and 2, both having a technically permissible maximum laden mass not exceeding 3,500 kg with positive ignition engines with the exclusion of mono-fuel gas vehicles, and to all vehicles of category 1-1 with positive ignition engines with the exclusion of mono-fuel gas vehicles.[[2]](#footnote-3)

3. Definitions

3.1. Test equipment

3.1.1. "*Accuracy*" means the difference between a measured value and a reference value, traceable to a national standard and describes the correctness of a result;

3.1.2. "*Calibration*" means the process of setting a measurement system's response so that its output agrees with a range of reference signals.

3.2. Hybrid electric vehicles

3.2.1. "*Charge-depleting operating condition*" means an operating condition in which the energy stored in the Rechargeable Electric Energy Storage System (REESS) may fluctuate but decreases on average while the vehicle is driven until transition to charge-sustaining operation;

3.2.2. "*Charge-sustaining operating condition*" means an operating condition in which the energy stored in the REESS may fluctuate but, on average, is maintained at a neutral charging balance level while the vehicle is driven;

3.2.3. "*Not off-vehicle charging hybrid electric vehicle*" (NOVC-HEV) means a hybrid electric vehicle that cannot be charged from an external source.

3.2.4. "*Off-vehicle charging hybrid electric vehicle*" (OVC-HEV) means a hybrid electric vehicle that can be charged from an external source.

3.2.5. "*Hybrid electric vehicle*" (HEV) means a hybrid vehicle where one of the propulsion energy energy converters is an electric machine.

3.2.6. "*Hybrid vehicle*" (HV) means a vehicle equipped with a powertrain containing at least two different categories of propulsion energy converters and at least two different categories of propulsion energy storage systems.

3.2.7. "*Not off-vehicle charging hybrid electric vehicle*" (NOVC-HEV) means a hybrid electric vehicle that cannot be charged from an external source.

3.2.8. "*Conventional ICE vehicle*" means…

3.3. Evaporative emission

3.3.1. "*Fuel tank system*" means the devices which allow storing the fuel, comprising the fuel tank, the fuel filler, the filler cap and the fuel pump when it is fitted in or on the fuel tank;

3.3.2. "*Fuel system*" means the components which store or transport fuel on board the vehicle and comprise the fuel tank system, all fuel and vapour lines, any non-tank mounted fuel pumps and the activated carbon canister;

3.3.3. "*Butane working capacity*" (BWC) means the measure of the ability of an activated carbon canister to adsorb and desorb butane from dry air or nitrogen under specified conditions;

3.3.4. "*BWC300*" means the butane working capacity after 300 cycles of fuel ageing cycles experienced;

3.3.5. "*Permeability factor*" (PF) means the factor determined from hydrocarbon permeation from fuel tank system over a period of time and used to determine the final evaporative emissions.

3.3.6. "*Monolayer tank*" means a fuel tank constructed with a single layer of material, excluding metal tank, but including fluorinated/sulfonated materials;

3.3.7. "*Multilayer tank*" means a fuel tank constructed with at least two different layered materials, one of which is a hydrocarbon barrier material;

3.3.8. "*Sealed fuel tank system*" means one of the following fuel tank system;

(a) a fuel tank system where the fuel vapours do not vent during parking over the 24-hour diurnal cycle defined in Appendix 2 to Annex 7 to Regulation No. 83-07 when performed with reference fuel defined in this Annex 2 of this UN GTR;

(b) a fuel tank system where the fuel vapours may vent during parking over the 24-hour diurnal cycle defined in Appendix 2 to Annex 7 to Regulation No. 83-07 when performed with reference fuel defined in this Annex 2 of this UN GTR and does not vent during a repeat of this 24-hour diurnal cycle;

3.3.9. "*Evaporative emissions*" means the hydrocarbon vapours lost from the fuel system of a motor vehicle other than those from exhaust emissions;

3.3.10. "*Mono-fuel gas vehicle*" means a mono-fuel vehicle that primarily runs on liquefied petroleum gas, natural gas/biomethane, or hydrogen but may also have a petrol system for emergency purposes or starting only, where the petrol tank does not contain more than 15 litres of petrol.

3.3.11. "*Depressurisation puff loss*" means hydrocarbons venting from the fuel tank system pressure relief exclusively through the vapour storage unit allowed by the system.

3.3.12. "D*epressurisation puff loss overflow*" are the hydrocarbons that pass through the vapour storage unit during depressurisation.

3.3.13. "*Fuel tank relief pressure*" is the minimum pressure value at which the sealed fuel tank system starts venting in response to purely pressure inside the tank.

3.3.14. "*Auxiliary canister*" is the canister used to measure depressurisation puff loss overflow.

4. Abbreviations

General abbreviations

|  |  |
| --- | --- |
| BWC | Butane working capacity |
| PF | Permeability factor |
| APF | Assigned permeability factor |
| OVC-HEV | Off-vehicle charging hybrid electric vehicle |
| WLTC | Worldwide light-duty test cycle |

5. General requirements

5.1. The vehicle and its components liable to affect the evaporative emissions shall be so designed, constructed and assembled as to enable the vehicle in normal use and under normal conditions of use such as humidity, rain, snow, heat, cold, sand, dirt, vibrations, wear, etc. to comply with the provisions of this gtr during its useful life determined by Contracting Parties.

5.1.1. This shall include the security of all hoses, joints and connections used within the evaporative emission control systems.

5.1.2. For vehicles with a sealed fuel tank system, this shall also include having a system which, just before refuelling, releases the tank pressure exclusively through a vapour storage unit which has the sole function of storing fuel vapour. This ventilation route shall also be the only one used in the situation that the tank pressure exceeds its safe working pressure.

5.2. The test vehicle shall be selected according to 5.5.2. of this UN GTR.

5.3. Vehicle testing condition

5.3.1. The types and amounts of lubricants and coolant for emissions testing shall be as specified for normal vehicle operation by the manufacturer.

5.3.2. The type of fuel for testing shall be as specified in Annex 2 to this UN GTR.

5.3.3. All evaporative emissions controlling systems shall be in working order.

5.3.4. The use of any defeat device is prohibited.

5.4. Provisions for electronic system security

5.4.1. Any vehicle with an emission control computer shall include features to deter modification, except as authorised by the manufacturer. The manufacturer shall authorise modifications if these modifications are necessary for the diagnosis, servicing, inspection, retrofitting or repair of the vehicle. Any reprogrammable computer codes or operating parameters shall be resistant to tampering and afford a level of protection at least as good as the provisions in ISO 15031-7 (March 15, 2001). Any removable calibration memory chips shall be potted, encased in a sealed container or protected by electronic algorithms and shall not be changeable without the use of specialized tools and procedures.

5.4.2. Computer-coded engine operating parameters shall not be changeable without the use of specialized tools and procedures (e.g. soldered or potted computer components or sealed (or soldered) enclosures).

5.4.3. Manufacturers may seek approval from the responsible authority for an exemption to one of these requirements for those vehicles that are unlikely to require protection. The criteria that the responsible authority will evaluate in considering an exemption shall include, but are not limited to, the current availability of performance chips, the high-performance capability of the vehicle and the projected sales volume of the vehicle.

5.4.4. Manufacturers using programmable computer code systems shall deter unauthorised reprogramming. Manufacturers shall include enhanced tamper protection strategies and write-protect features requiring electronic access to an off-site computer maintained by the manufacturer. Methods giving an adequate level of tamper protection will be approved by the responsible authority.

5.5. Evaporative emission family

5.5.1. Only vehicles that are identical for the following parameters (a) to (d) and are similar or, where applicable, within the stated tolerance for the following parameters (e) and (f) may be part of the same evaporative emission family:

(a) Fuel tank system material and construction;

(b) Vapour hose material, fuel line material and connection technique;

(c) Sealed tank or non-sealed tank system;

(d) Fuel tank relief valve setting (air ingestion and relief);

(e) Canister butane working capacity (BWC300) within a 10 per cent range (for canisters with the same type of charcoal, the volume of charcoal shall be within 10 per cent of that for which the BWC300 was determined);

(f) Purge control system (for example, type of valve, purge control strategy).

5.5.2. The vehicle shall be considered to produce worst-case evaporative emissions and shall be used for testing if it has the largest ratio of fuel tank capacity to canister butane working capacity within the family. If the ratio is identical, the lowest purge volume over the single purge cycle described in paragraphs 6.5. and 6.5.6. of Annex 1 shall be considered for the vehicle selection. The vehicle selection shall be agreed in advance by the responsible authority.

5.5.3. The use of any innovative system calibration, configuration, or hardware related to the evaporative control system places the vehicle model in a different family.

5.6 The responsible authority shall not grant type approval if the information provided is insufficient to demonstrate that the evaporative emissions are effectively limited during the normal use of the vehicle. The responsible authority may audit or witness any part of the tests described in Annex 1, or if there is reasonable doubt regarding the efficiency of the evaporative controls, request to repeat any part of the tests described in Annex 1.

6. Performance requirements

6.1. Limit values

The following limit values shall apply:

(a) For Contracting Parties which adopt the calculation defined in paragraph 7.1. of Annex 1, the limit value shall be 2.0 g/test;

(b) For Contracting Parties which adopt the alternative calculation defined in paragraph 7.2. of Annex 1, the limit value shall be determined by the Contracting Party.

6.2. Testing

Testing shall be performed according to the Type 4 test as described in Annex 1 using the appropriate fuel as described in Annex 2.

Annex 1

Type 4 test procedures and test conditions

1. Introduction

This annex describes the procedure for the Type 4 test which determines the emission of hydrocarbons by evaporation from the fuel systems of vehicles.

2. Technical requirements

2.1. The procedure includes the evaporative emissions test and two additional tests, one for the ageing of carbon canisters, as described in paragraph 5.1. of this annex, and one for the permeability of the fuel storage system, as described in paragraph 5.2. of this annex. The evaporative emissions test (Figure A1/5a and Figure A1/5b) determines hydrocarbon evaporative emissions as a consequence of diurnal temperature fluctuations and hot soaks during parking.

2. 2. In the case that the fuel system contains more than one carbon canister, all references to the term "canister" in this UN GTR will apply to each canister.

3. Vehicle and fuel

3.1. Vehicle

3.1.1. The vehicle shall be in good mechanical condition and have been run-in and driven at least 3,000 km before the test. For the purpose of the determination of evaporative emissions, the mileage and the age of the vehicle used for certification shall be recorded. The evaporative emission control system shall be connected and have been functioning correctly during the run-in period. A carbon canister aged according to the procedure set out in paragraph 5.1. of this annex shall be used.

3.1.2. The Type 4 test shall be performed with the vehicle which produces the worst evaporative emissions within the evaporative emission family according to paragraph 5.5. of this UN GTR.

3.2. Fuel

The appropriate reference fuel as defined in Annex 2 shall be used for testing. For canister ageing, fuel specified in paragraph 5.1.3.1.1.1. of this annex shall be used.

4. Test equipment

4.1. Chassis dynamometer

The chassis dynamometer shall meet the requirements of paragraph 2. of Annex 5 to UN GTR No. 15.

4.2. Evaporative emission measurement enclosure

The evaporative emission measurement enclosure shall meet the requirements of paragraph 4.2. of Annex 7 to the 07 series of amendments to Regulation No. 83 (Regulation No. 83-07).

4.3. Analytical systems

The analytical systems shall meet the requirements of paragraph 4.3. of Annex 7 to Regulation No. 83-07. Continuous measuring of hydrocarbons is not mandatory unless the fixed volume type enclosure is used.

4.4. Temperature recording system

The temperature recording shall meet the requirements of paragraph 4.5. of Annex 7 to Regulation No. 83-07.

4.5. Pressure recording system

The pressure recording shall meet the requirements of paragraph 4.6. of Annex 7 to Regulation No. 83-07, except that the accuracy and resolution of the pressure recording system defined in paragraph 4.6.2. of Annex 7 to Regulation No. 83-07 shall be:

(a) Accuracy: ±0.3 kPa

(b) Resolution: 0.025 kPa

4.6. Fans

The fans shall meet the requirements of paragraph 4.7. of Annex 7 to Regulation No. 83-07, except that the capacity of the blowers shall be 0.1 to 0.5 m³/sec instead of 0.1 to 0.5 m³/min.

4.7. Calibration gases

The gases shall meet the requirements of paragraph 4.8. of Annex 7 to Regulation No. 83-07.

4.8. Additional Equipment

The additional equipment shall meet the requirements of paragraph 4.9. of Annex 7 to Regulation No. 83-07.

4.9. Auxiliary canister

[Text expected from Delphi]4.10 Scale to measure mass of the canister of vehicle and the auxiliary canister

The scale shall have an accuracy of ±0.02 g.

5. Test procedure

5.1. Canister bench ageing

Before performing the hot soak and diurnal losses sequences, the canister shall be aged according to the procedure described in Figure A1/1.

Figure A1/1

**Canister bench ageing procedure**

Test start

Select new canister sample.

1. Temperature conditioning test

According to paragraph 5.1.1. of this annex.

2. Canister vibration conditioning test

According to paragraph 5.1.2. of this annex.

3. Fuel ageing for 300 cycles

According to paragraph 5.1.3. of this annex.

{

50 times

5.1.1. Temperature conditioning test

The canister shall be cycled between temperatures from -15 °C to 60 °C in a dedicated temperature enclosure with 30 minutes of stabilisation at -15 °C and 60 °C. Each cycle shall last 210 minutes (see Figure A1/2).

The temperature gradient shall be as close as possible to 1 °C/min. No forced air flow should pass through the canister.

The cycle shall be repeated 50 times consecutively. In total, this procedure lasts 175 hours.

Figure A1/2

**Temperature conditioning cycle**



5.1.2. Canister vibration conditioning test

Following the temperature ageing procedure, the canister shall be shaken vertically with the canister mounted as per its orientation in the vehicle with an overall Grms > 1.5 m/sec2 with a frequency of 30 ±10 Hz. The test shall last 12 hours.

5.1.3. Canister fuel ageing test

5.1.3.1. Fuel ageing for 300 cycles

5.1.3.1.1. After the temperature conditioning test and vibration test, the canister shall be aged with a mixture of market fuel as specified in paragraph 5.1.3.1.1.1. of this annex and nitrogen or air with a 50 ±15 per cent fuel vapour volume. The fuel vapour fill rate shall be 60 ±20 g/h.

The canister shall be loaded to the corresponding breakthrough. Breakthrough shall be considered accomplished when the cumulative quantity of hydrocarbons emitted equals 2 grams. As an alternative, loading shall be deemed completed when the equivalent concentration level at the vent outlet reaches 3,000 ppm.

5.1.3.1.1.1. The market fuel used for this test shall fulfil the same requirements as a reference fuel with respect to:

(a) Density at 15 °C;

(b) Vapour pressure;

(c) Distillation (70 °C, 100 °C, 150 °C);

(d) Hydrocarbon analysis (olefins, aromatics, benzene only);

(e) Oxygen content;

(f) Ethanol content.

5.1.3.1.2. The canister shall be purged with 25 ±5 litres per minute with emission laboratory air until 300 bed volume exchanges are reached.

The canister shall be purged between 5 and 60 minutes after loading.

5.1.3.1.3. The procedures set out in paragraphs 5.1.3.1.1. and 5.1.3.1.2. of this annex shall be repeated 300 times. The canister aged with 300 fuel ageing cycles shall be considered to be stabilised.

5.1.3.1.4 The procedure to measure the butane working capacity (BWC) with respect to the evaporative emission family in paragraph 5.5. of this UN GTR shall consist of loading the canister with butane after 300 fuel ageing cycle according to paragraph 5.1.6.3. of Annex 7 to Regulation No. 83-07 until breakthrough. The butane loading shall be repeated minimum 5 times. The BWC shall be recorded after the loading. The canister shall be subsequently purged according paragraph 5.1.3.1.2. of this annex. The BWC300 shall be calculated as the average of the last 5 BWCs.

5.1.3.2. If an aged canister is provided by a supplier, the manufacturer shall inform the responsible authority in advance of the ageing process to enable witnessing any part of the ageing in the supplier’s facilities.

5.1.3.3. The manufacturer shall provide the responsible authority a test report including at least the following elements:

(a) Type of activated carbon;

(b) Loading rate;

(c) Fuel specifications;

5.2. Determination of the permeability factor (PF) of the fuel tank system (Figure A1/4)

Figure A1/3

**Determination of the PF**

Test start

Fill the tank to 40 ±2 per cent of its nominal capacity with fresh reference fuel

Soak for 3 weeks at 40 °C ±2 °C

Measurement of HC in the same conditions as in the 1st day of diurnal emission test :

HC 3w

Soak for the remaining 17 weeks at 40 °C ±2 °C

Measurement of HC in the same conditions as in the 1st day of diurnal emission test:

HC 20w

Permeability Factor

= HC 20w - HC3w

Drain and fill the tank to 40 per cent of its nominal capacity with reference fuel

Drain and fill the tank with reference fuel at 40 per cent of its nominal capacity

The fuel tank system representative of a family shall be selected and mounted on a rig, and subsequently soaked with reference fuel for 20 weeks at 40 °C ±2 °C. The orientation of the fuel storage system on the rig shall be as that in the vehicle.

5.2.1. The tank shall be filled with fresh reference fuel at a temperature of 18 °C ±2 °C. The tank shall be filled to 40 ±2 per cent of the nominal tank capacity. The rig with the fuel tank system shall be placed in a room with a controlled temperature of 40 °C ±2 °C for 3 weeks.

5.2.2. At the end of the third week, the tank shall be drained and refilled with fresh reference fuel at a temperature of 18 °C ±2 °C to 40 ±2 per cent of the nominal tank capacity.

Within 6 to 36 hours, the rig with the fuel tank system shall be placed in an enclosure. The last 6 hours of this period shall be at an ambient temperature of 20 °C ±2 °C. In the enclosure, a diurnal procedure shall be performed over a first period of 24 hours of the procedure described in paragraph 6.5.9. of this annex. The fuel tank system shall be vented to the outside of the enclosure to eliminate the possibility of the tank venting emissions being counted as permeation. The HC emissions shall be measured and the value shall be recorded as HC3W.

5.2.3. The rig with the fuel tank system shall be placed again in a room with a controlled temperature of 40 °C ±2 °C for the remaining 17 weeks.

5.2.4. At the end of the seventeenth week, the tank shall be drained and refilled with fresh reference fuel at a temperature of 18 °C ±2 °C at 40 ±2 per cent of the nominal tank capacity.

Within 6 to 36 hours, the rig with the fuel tank system shall be placed in an enclosure. The last 6 hours of this period shall be at an ambient temperature of 20 °C ±2 °C. In the enclosure, a diurnal procedure shall be performed over a first period of 24 hours of the procedure described according to paragraph6.5.9. of this annex. The fuel tank system shall be vented to the outside of the enclosure to eliminate the possibility of the tank venting emissions being counted as permeation. The HC emissions shall be measured and the value shall be recorded as HC20W.

5.2.5. The PF is the difference between HC20W and HC3W in g/24h calculated to 3 significant digits using the following equation:

5.2.6. If the PF is determined by a supplier, the vehicle manufacturer shall inform the responsible authority in advance of the determination to allow witness check in the supplier’s facility.

5.2.7. The manufacturer shall provide the responsible authority a test report containing at least the following:

(a) A full description of the fuel storage system tested, including information on the type of tank tested, whether the tank is monolayer or multilayer, and which types of materials are used for the tank and other parts of the fuel storage system;

(b) The weekly mean temperatures at which the ageing was performed;

(c) The HC measured at week 3 (HC3W);

(d) The HC measured at week 20 (HC20W);

(e) The resulting permeability factor (PF).

5.2.8. As an exception to paragraphs 5.2.1. to 5.2.7. inclusive of this annex, a manufacturer using multilayer tanks or metal tanks may choose to use an APF instead of the complete measurement procedure mentioned above:

APF multilayer/metal tank = 120 mg /24 h

Where the manufacturer chooses to use an APF, the manufacturer shall provide the responsible authority a declaration in which the type of tank is clearly specified as well as a declaration of the type of materials used.

6. Test procedure for measurement of hot soak and diurnal losses

6.1. Vehicle preparation

The vehicle shall be prepared in accordance to paragraphs 5.1.1. and 5.1.2. of Annex 7 to Regulation No. 83-07. At the request of the manufacturer and with the approval of the responsible authority, non-fuel background emission sources (e.g. paint, adhesives, plastics, fuel/vapour lines, tyres, and other rubber or polymer components) may be reduced to vehicle background levels before testing (e.g. baking of tyresat temperatures of 50 °C or higher for appropriate periods, baking of vehicle, draining washer fluid).

6.2. Mode selections and gear shift prescriptions

6.2.1. For vehicles with manual shift transmissions, the gear shift prescriptions specified in UN GTR No. 15 shall apply.

6.2.2. In the case of conventional ICE vehicles, the mode shall be selected according to paragraph 2.6.5.3. to Annex 6 to UN GTR No. 15.

6.2.3. In the case of NOVC-HEV and OVC-HEV the mode shall be selected according to Appendix 6 to Annex 8 of UN GTR No. 15.

6.3. Test conditions

The tests included in this UN GTR shall be performed using the test conditions specific to the interpolation family vehicle L [or H] with the lowest [or highest] cycle energy demand of all the interpolation families included in the evaporative emission family being considered.

#### For the driving events included in this UN GTR, considering each of the interpolation families included in the evaporative emission family being tested, the test conditions specific to the vehicle L [or H] with the lowest [or highest] cycle energy demand shall be used.

6.4 Selection of the test procedure

6.4.1. The test procedure shall be selected according to the flow chart described in Figure A1/4.

Figure A1/4

**Selection process**

6.5. Test procedure for non-sealed fuel tank system

Yes

No

“*Sealed fuel tank system*”?

Fuel tank relief pressure ≧ 30 kPa

Fuel tank relief pressure ≧ 30 kPa

Use paragraph 6.6. of UN GTR

Use paragraph 6.7. of UN GTR

Use paragraph 6.6.1. of UN GTR

Use paragraph 6.5. of UN GTR

Use paragraph 6.6.2. of UN GTR

Use paragraph 6.7.2. of UN GTR

Use paragraph 6.7.1. of UN GTR

Yes

Yes

No

No

Manufacturer’s choice of test procedure

Figure A1/5a

**Test procedure for non-sealed fuel tank system**

Start

2nd day diurnal : MD2 (8)

Calculation

End

6 to 36 hours

Max 5 min

(1) Fuel temp. 18 °C ±2 °C

40 per cent ±2 per cent of nominal tank capacity

(2) Low–Medium–High– Medium phase for Class 2 and 3 vehicles.

Two times of Low–Medium– Low phase for Class 1 vehicles.

Start temp. = 23 °C ±3 °C

(3) Soak at 23 °C ±3 °C

(4) for OVC-HEV only

(5) Within 7 minutes of the end of the test drive and within 2 minutes of the engine being switched off.

(6) Min. temp. = 23 °C

Max. temp. = 31 °C

Duration = 60 min ±0.5 min

(7) Soak at 20 °C ±2 °C

(8) Start temp. = 20 °C

Max. temp. = 35 °C

Delta temp. =15 °C

Duration = 24 hours

Number of diurnals = 2 days

Max 7 min (5)

Load aged canister to 2 g breakthrough

Soak (7)

6 to 36 hours

Hot soak test: M HS (6)

1st day diurnal : MD1 (8)

Start soaking(3)

12 h to 36 h

Fuel drain and refill (1)

Max 1 hour

Dynamometer test (2)

Start REESS charge (4)

Preconditioning drive (2)

Pre-conditioning drive (2)

6.5.1. Fuel drain and refill

The fuel tank of the vehicle shall be emptied. This shall be done so as not to abnormally purge or abnormally load the evaporative control devices fitted to the vehicle. Removal of the fuel cap is normally sufficient to achieve this. The fuel tank shall be refilled with test fuel at a temperature of 18 °C ±2 °C to 40 ±2 per cent of the tank's nominal capacity.

6.5.2. Preconditioning drive

After completing the fuel drain and refilling following soaking for a minimum of 6 hours and a maximum of 36 hours at 23 °C ±3 °C, the vehicle shall be placed on a chassis dynamometer and driven over the following phases of the cycle described in Annex 1 of UN GTR No. 15:

a) For Class1 vehicles:  
 low, medium, low, low, medium, low

b) For Class 2 and 3 vehicles:  
 low, medium, high, medium

For OVC-HEV, preconditioning drive shall be performed under the charge-sustaining operating condition as defined in paragraph 3.3.6. of UN GTR No. 15.

Exhaust emissions need not be measured during this operation.

6.5.3. Soak

Within five minutes of completing preconditioning, the vehicle shall be parked for a minimum of 12 hours and a maximum of 36 hours at 23 °C ±3 °C. The engine oil and coolant temperatures shall have reached a temperature within ±3 °C of the area before the canister breakthrough loading may begin.

6.5.4. REESS charge

For OVC-HEV, the REESS shall be fully charged according to the charging requirements described in paragraph 2.2.3. of Appendix 4 to Annex 8 to UN GTR No.15 during soaking.

6.5.5. Canister loading

The canister aged according to the sequence described in paragraph 5.1. of this annex shall be loaded to breakthrough according to the procedure described in paragraph 5.1.4. of Annex 7 to Regulation No. 83-07.

Within one hour after completing canister loading, the vehicle shall be placed on the chassis dynamometer.

6.5.6. Dynamometer test

The vehicle shall be driven over the cycles as described in paragraph 6.5.2. a) or b) of this annex. OVC-HEVs shall be operated in charge-depleting operating condition. The engine shall be subsequently shut off. Exhaust emissions may be sampled during this operation but the results shall not be used for the purpose of exhaust emission type approval.

After 6.5.5. the vehicle shall be placed on a chassis dynamometer and driven over the following phases of the cycle described in Annex 1 of UN GTR No. 15:

a) For Class1 vehicles: low, medium, low, low, medium, low

b) For Class 2 and 3 vehicles of Classes 2 and 3: low, medium, high, medium

For OVC-HEV, dynamometer test shall be performed under the charge-depleting operating condition as defined in paragraph 3.3.6. of UN GTR No. 15.

The engine shall be subsequently shut off. Exhaust emissions may be sampled during this operation but the results shall not be used for the purpose of exhaust emission type approval.

6.5.7. Hot soak evaporative emissions test

After the dynamometer test, the hot soak evaporative emissions test shall be performed in accordance to paragraph 5.5. of Annex 7 to Regulation No. 83-07. The hot soak losses result shall be calculated according to paragraph 6. of Annex 7 to Regulation No. 83-07 and recorded as MHS.

6.5.8. Soak

After the hot soak evaporative emissions test, the test vehicle shall be soaked for not less than 6 hours and not more than 36 hours between the end of the hot soak test and the start of the diurnal emission test. For at least 6 hours of this period the vehicle shall be soaked at 20 °C ±2 °C.

6.5.9. Diurnal testing

6.5.9.1. The test vehicle shall be exposed to two cycles of ambient temperature according to the profile specified for the diurnal emission test in Appendix 2 to Annex 7 to Regulation No. 83-07 with a maximum deviation of ±2 °C at any time. The average temperature deviation from the profile, calculated using the absolute value of each measured deviation, shall not exceed ±1 °C. Ambient temperature shall be measured and recorded at least every minute. Temperature cycling begins when time Tstart = 0, as specified in paragraph 6.5.9.6. of this annex.

6.5.9.2. The enclosure shall be purged for several minutes immediately before the test until a stable background is obtained. The chamber mixing fan(s) shall also be switched on at this time.

6.5.9.3. The test vehicle, with the engine shut off and the test vehicle windows and luggage compartment(s) opened, shall be moved into the measuring chamber. The mixing fan(s) shall be adjusted in such a way as to maintain a minimum air circulation speed of 8 km/h under the fuel tank of the test vehicle.

6.5.9.4. The hydrocarbon analyser shall be zeroed and spanned immediately before the test.

6.5.9.5. The enclosure doors shall be closed and sealed gas-tight.

6.5.9.6. Within 10 minutes of closing and sealing the doors, the hydrocarbon concentration, temperature and barometric pressure shall be measured to give initial readings of hydrocarbon concentration in the enclosure CHCi, barometric pressure Pi and ambient chamber temperature Ti for the diurnal testing. Tstart= 0 starts at this time.

6.5.9.7. The hydrocarbon analyser shall be zeroed and spanned immediately before the end of each emission sampling period.

6.5.9.8. The end of the first and second emission sampling period shall occur 24 hours ±6 minutes and 48 hours ±6 minutes, respectively, after the beginning of the initial sampling, as specified in paragraph 6.5.9.6. of this annex. The elapsed time shall be recorded.

At the end of each emission sampling period, the hydrocarbon concentration, temperature and barometric pressure shall be measured to give the readings of hydrocarbon concentration in the enclosure CHCf, barometric pressure Pf and ambient chamber temperature Tf for the diurnal. The diurnal results shall be calculated according to paragraph 6. of Annex 7 of UN/ECE Regulation No. 83-07. The value obtained from the first 24 hours shall be recorded as MD1. The value obtained from the second 24 hours shall be recorded as MD2.

6.6. Test procedure option 1 for a sealed fuel tank system

Figure A1/5b

**The evaporative emission test with one series of test procedure**

Start

2nd day diurnal : MD2 (11)

Calculation

End

(1) Fuel temp.: 18 °C ±2 °C

40 per cent ± 2 per cent of nominal tank capacity

(2) Low–Medium–High– Medium phase for Class 2 and 3 vehicles.

Two times of Low–Medium– Low phase for Class 1 vehicles.

Start temp. = 23 °C ±3 °C

(3) Soak at 23 °C ±3 °C

(4) for OVC-HEV only

(5) Fuel temp.: 18 °C ±2 °C  
15 per cent ± 2 per cent of nominal tank capacity

(6) Soak at 20 °C ±2 °C

(7) Up to 85 per cent fuel consumption equivalent defined in 6.4.1.4.1. in this Annex.

(8) Temperature profile is the first 11 hours portion specified in Appendix 2 to Annex 7 to Regulation No. 83-07.

(9) Overflow puff loss mass shall be measured by either connecting an auxiliary canister or using a SHED.

(10) Within 7 minutes of the end of the test drive and within 2 minutes of the engine being switched off.

(10) Min. temp. = 23 °C

Max. temp. = 31 °C

Duration = 60 min ±0.5 min

(11) Start temp. = 20 °C

Max. temp. = 35 °C

Delta temp. =15 °C

Duration = 24hours

Number of diurnals = 2 days

Max 7 min (10)

Dynamometer test (2)

Hot soak test : MHS(10)

1st day diurnal : MD1 (11)

Soak (6)

Load aged canister to 2g breakthrough

Canister purge (7)

Soak in enclosure (8)

Tank pressure relief / puff loss loading (9)

Fuel refill (1)

Start REESS charge (4)

Fuel drain and refill (5)

Fuel tank pressure relief

6 to 36 hours

Preconditioning drive (2)

Start soaking (3)

Max 15 min

Soak (3)

Fuel drain and refill (1)

6 to 36 hours

6 to 36 hours

6 to 36 hours

Soak (6)

6.6.1. In case that the fuel tank relief pressure is greater than or equal to 30 kPa

6.6.1.1. The test shall be performed as described in paragraphs 6.5.1. to 6.5.4. inclusive of this annex.

6.6.1.2. Second fuel drain and refill

Within one hour after preconditioning drive, the fuel tank of the vehicle shall be emptied. This shall be done so as not to abnormally purge or abnormally load the evaporative control devices fitted to the vehicle. Removal of the fuel cap is normally sufficient to achieve this, otherwise the canister shall be disconnected. The fuel tank shall be refilled with test fuel at a temperature of 18 °C ±2 °C to 15 ±2 per cent of the tank's nominal capacity.

6.6.1.3. Relief of fuel tank pressure

The vehicle shall be soaked for stabilization for 6 to 36 hours at an ambient temperature of 20 °C ±2 °C. The tank pressure shall be subsequently released so as not to abnormally raise the inside pressure of the fuel tank. This may be done by opening the fuel cap of the vehicle. Regardless of the method of depressurisation, the vehicle shall be returned to its original condition within 1 minute.

6.6.1.4. Canister loading and purge

The canister aged according to the sequence described in paragraph 5.1. of this annex shall be loaded to breakthrough according to the procedure described in paragraph 5.1.6. of Annex 7 of UN/ECE Regulation No. 83-07, and shall be subsequently purged with air with 25 ±5 litres per minute. The volume of air shall not exceed a maximum equivalent to 85 per cent fuel consumption of nominal fuel tank capacity calculated as described in paragraph 6.6.1.4.1. of this annex. The canister shall be mounted correctly in the vehicle, if applicable.

6.6.1.4.1. Determination of maximum purge volume

The maximum purge amount shall be determined by the following equation. In the case of OVC-HEVs, the vehicle shall be operated in charge-sustaining operating condition.

where:

is the accumulated measured purge volume over the single purge cycle described in the paragraph 6.5.2. of this annex to nearest 0.1 litres, l;

is the manufacturer’s nominal fuel tank capacity, l;

is the fuel consumption over the single purge cycle described in paragraph 6.5.2. of this annex and which may be measured in either warm or cold start condition, l/100 km. For OVC-HEVs and NOVC-HEVs, fuel consumption shall be calculated according to 4.2.1. of Annex 8 of UN GTR 15;

is the theoretical distance of a single purge cycle described in paragraph 6.5.2. of this annex to the nearest 0.1 km, km.

6.6.1.5. Preparation of canister depressurisation puff loss loading

After completing canister loading and purging, the test vehicle shall be moved into an enclosure, either a SHED or an appropriate climatic chamber. It shall be demonstrated that the system has no leak and the pressurization is performed in a normal way (e.g. by means of pressure sensor on the vehicle). The test vehicle shall be subsequently exposed to ambient temperature according to the first 11-hour profile specified for the diurnal emission test in Appendix 2 to Annex 7 to Regulation No. 83-07 with a maximum deviation of ±2 °C at any time. The average temperature deviation from the profile, calculated using the absolute value of each measured deviation, shall not exceed ±1 °C. Ambient temperature shall be measured and recorded at least every 10 minutes.

6.6.1.6. Canister puff loss loading

6.6.1.6.1. In case of using an auxiliary canister to measure depressurisation puff loss over flow

Within 15 minutes after the ambient temperature has reached 35 °C, the test vehicle shall be taken from an enclosure and the tank relief valve shall be opened to load the canister.

6.6.1.6.2. In case of using a SHED to measure depressurisation puff loss overflow

Within 15 minutes after the ambient temperature has reached 35 °C, the tank relief valve shall be opened to load the canister.

6.6.1.6.3. Fuel tank depressurisation before refuelling

The manufacturer shall ensure that the refuelling operation cannot be initiated before the sealed fuel tank system is fully depressurised to reach a pressure less than 2.5 kPa above ambient pressure. At the request of the responsible authority, the manufacturer shall provide detailed information or demonstrate proof of operation (e.g. by means of pressure sensor on the vehicle). Any other technical solution may be allowed provided that a safe refuelling operation is ensured and that no excessive emissions are released to the atmosphere before the refuelling device is connected to the vehicle according to the test procedure 5.4.1.5. in Annex 1 of this UN GTR.

6.6.1.7. Measurement of depressurisation puff loss overflow

6.6.1.7.1. Any deprssurisation puff loss overflow from the vehicle canister shall be measured by using an auxiliary carbon canister connected directly at the outlet of the vehicle vapour storage unit. The connection tube shall be as short as possible. The auxiliary canister shall be well purged with dry air prior to loading and shall be weighed before and after the procedure described in paragraph 6.6.1.6. of this annex. The increase in weight in grams of the auxiliary canister shall be recorded as STPL (Sealed Tank Puff Loss).

6.6.1.7.2. Alternatively, the depressurisation puff loss overflow from the vehicle canister during its depressurisation or before the refuelling operation can be started, may be measured also using a SHED.

Within 15 minutes after the ambient temperature has reached 35 °C as described in 6.6.1.6.2. of this annex, the chamber shall be sealed and the measurement procedure started.

The hydrocarbon analyser shall be zeroed and spanned. Immediately after the hydrocarbon concentration, temperature and barometric pressure shall be measured to give the initial readings CHCi, Pi and Ti for the sealed tank puff loss determination.

At the end of the procedure prescribed by the manufacturer to enable the refuelling operation and when the tank has reached a condition enabling the refuelling operation, the hydrocarbon concentration in the chamber shall be measured after 60 ± 5 seconds. The temperature and the barometric pressure are also measured. These are the final readings CHCf, Pf and Tf for the sealed tank puff loss.

The sealed tank puff loss result shall be calculated as follows:

where:

STPL is the sealed tank puff loss, grams;

MHC is the mass of hydrocarbons, grams;

MHC,out is the mass of hydrocarbons exiting the enclosure in the case of fixed volume enclosures for diurnal emission testing, grams;

MHC,in is the mass of hydrocarbon entering the enclosure in the case of fixed volume enclosures for diurnal emission testing, grams;

CHC is the measured hydrocarbon concentration in the enclosure, ppm volume in C1 equivalent;

V is the net enclosure volume in cubic metres corrected for the volume of the vehicle with the windows and the luggage compartment open. If the volume of the vehicle is not known, a volume of 1.42 m3 shall be subtracted,

T is the ambient chamber temperature, in K;

P is the barometric pressure, kPa;

H/C is the hydrogen to carbon ratio a constant value and is taken to be 2.33;

k is 1.2 × (12 + H/C); i is the initial reading;

f is the final reading;

6.6.1.7.3. The change in weight of the auxiliary canister or the SHED measurement after the depressurisation compared to before depressurisation shall be less than 0.5 gram.

The change in weight of the auxiliary canister or the SHED measurement after the depressurisation compared to before the temperature increase shall be less than 0.5 gram.

6.6.1.8. Fuel refill and soaking

After completiin puff loss loading, the vapour storage unit shall be disconnected and the vehicle shall be soaked at 23 ±3 °C for 6 to 36 hours. The fuel tank of the vehicle shall be refilled up to 40 ±2 per cent of the tank's nominal capacity with test fuel at a temperature of 18 °C ±2 °C. The manufacturer may choose to drain the fuel before refill. The vehicle shall be subsequently parked for a minimum of 6 hours to a maximum of 36 hours in the soak area.

6.6.1.9. The tank pressure shall be subsequently released so as not to abnormally raise the inside pressure of the fuel tank. This may be done by opening the fuel cap of the vehicle. Regardless of the method of depressurisation, the vehicle shall be returned to its original condition within 1 minute. After this action, the vapour storage unit shall be connected again.

6.6.1.10. The procedures in paragraphs 6.5.6. to 6.5.9.8. inclusive of this annex shall be followed.

6.6.2. In case that the fuel tank relief pressure is lower than 30 kPa

The test shall be performed as described in paragraphs 6.6.1.1. to 6.6.1.9. inclusive of this annex with one execption. The ambient temperature described in 6.5.9.1. of this annex shall be modified according to the profile specified in Table A1/1 of this annex for the diurnal emission test.

Table A1/1

**Ambient temperature profile of the alternative sequence for sealed fuel tank system**

|  |  |
| --- | --- |
| Time (hours) | Temperature (degrees C) |
| 0/24 | 20.0 |
| 1 | 20.4 |
| 2 | 20.8 |
| 3 | 21.7 |
| 4 | 23.9 |
| 5 | 26.1 |
| 6 | 28.5 |
| 7 | 31.4 |
| 8 | 33.8 |
| 9 | 35.6 |
| 10 | 37.1 |
| 11 | 38.0 |
| 12 | 37.7 |
| 13 | 36.4 |
| 14 | 34.2 |
| 15 | 31.9 |
| 16 | 29.9 |
| 17 | 28.2 |
| 18 | 26.2 |
| 19 | 24.7 |
| 20 | 23.5 |
| 21 | 22.3 |
| 22 | 21.0 |
| 23 | 20.2 |

6.7 Test procedure option 2 for a sealed fuel tank system

6.7.1 In case that the fuel tank relief pressure is greater than or equal to 30 kPa

6.7.1.1. The test shall be performed as described in paragraphs 6.5.1. to 6.5.4. inclusive of this annex.

6.7.1.2. The canister shall be aged according to the sequence described in paragraph 5.1. of this annex and shall be preconditioned according to paragraph 6.6.1.4. of this annex.

6.7.1.3. After completing canister preconditioning, the canister shall be loaded according to the procedure described in paragraph 5.1.6. of Annex 7 to Regulation No. 83-07 with exemption of loading mass. At the request of manufacturer, the reference fuel may alternatively be used instead of butane. Total loading mass shall be determined according to paragraph 6.7.3. of this annex.

Within one hour after completing canister loading, the vehicle shall be placed on the chassis dynamometer.

6.7.1.3.1. At the option of the manufacturers, the procedure defined in paragraphs 6.7.1.2. and 6.7.1.3. of this annex may be omitted. In this case, paragraph 6.5.5. of this annex shall be followed.

6.7.1.4. The procedures in paragraphs 6.5.6. to 6.5.9.8. inclusive of this annex shall be followed.

6.7.2. In case that the fuel tank relief pressure is lower than 30 kPa

The test shall be performed as described in paragraphs 6.7.1.1. to 6.7.1.4. inclusive of this annex with one exception. The ambient temperature described in 6.5.9.1. of this annex shall be modified according to the profile specified in Table A1/1 of this annex for the diurnal emission test.

6.7.3. Measurement of depressurisation puff loss loading mass

6.7.3.1. The vehicle shall be soaked for 6 to 36 hours at 23 °C ±3 °C.6.7.3.2. The procedures in paragraphs 6.6.1.2. to 6.6.1.6. inclusive of this annex shall be performed. The depressurisation puff loss loading mass is defined by the vehicle canister weight difference before and after paragraph 6.6.1.6.

6.7.3.3. The depressurisation puff loss overflow from the vehicle canister shall be measured according to paragraph 6.6.1.7. in this annex.

7. Calculation

7.1. The result of (MHS + MD1 + MD2 + 2 × PF) shall be below the limit defined in paragraph 6.1.(a) of this UN GTR.

In case of sealed tanks, the result of (STPL+ MHS + MD1 + MD2 + 2 × PF) shall be below the limit defined in paragraph 6.1.(a) of this UN GTR.

7.2. At the option of the Contracting Party, the following alternative calculation may be used.

The result of (MHS + MD\_max + PF) shall be below the limit defined in paragraph 6.1.(b) of this UN GTR. The MD\_max shall be either MD1 or MD2, whichever generates the higher emission.

8. Test report The test report shall contain at least the following:

(a) Description of the soak periods, including time and mean temperatures;

(b) Description of aged canister used and reference to exact ageing report;

(c) Mean temperature during the hot soak test;

(d) Measurement during hot soak test, HSL;

(e) Measurement of first diurnal, DL1st day;

(f) Measurement of second diurnal, DL2nd day;

(g) Final evaporative test result, calculated according to paragraph 7. of this annex.

Annex 2

Reference fuels

1. As there are regional differences in the market specifications of fuels, regionally different reference fuels need to be recognised. Contracting Parties may select their reference fuels either according to Annex 3 to UN GTR No. 15. or according to paragraph 2. of this annex.

2. Specification of reference fuel for testing for mutual recognition

The reference fuel listed in Table A2/1 is designed to be used as the reference fuel for mutual recognition under the rules of the 1998 Agreement.

3. Specification of reference fuel for regional testing

The reference fuel listed in Annex 3 to UN GTR No. 15. may be used for this purpose.

Table A2/1

| *Parameter* | *Unit* | *Limits* | | *Test method* |
| --- | --- | --- | --- | --- |
| *Minimum* | *Maximum* |
| Research octane number, RON |  | 95.0 | 98.0 | EN ISO 5164  JIS K2280 |
| Density at 15 °C | kg/m3 | 743.0 | 756.0 | EN ISO 12185  JIS K2249-1,2,3 |
| Vapour pressure | kPa | 56.0 | 60.0 | EN 13016-1  JIS K2258-1,2 |
| Distillation: |  |  |  |  |
| – evaporated at 70 °C | % v/v | 34.0 | 46.0 | EN ISO 3405 |
| – evaporated at 100 °C | % v/v | 54.0 | 62.0 | EN ISO 3405 |
| – evaporated at 150 °C | % v/v | 86.0 | 94.0 | EN ISO 3405 |
| Hydrocarbon analysis: |  |  |  |  |
| – olefins | % v/v | 6.0 | 13.0 | EN 22854 |
| – aromatics | % v/v | 25.0 | 32.0 | EN 22854 |
| – benzene | % v/v | - | 1.00 | EN 22854 EN 238  JIS K2536-2,3,4 |
| Oxygen content | % m/m | 3.3 | 3.7 | EN 22854  JIS K2536-2,4,6 |
| Sulphur content | mg/kg | — | 10 | EN ISO 20846  EN ISO 20884  JIS K2541-1,2,6,7 |
| Lead content | mg/l | Not detected | | EN 237  JIS K2255 |
| Ethanol | % v/v | 9.0 | 10.0 | EN 22854  JIS K2536-2,4,6 |
| MTBE |  | Not detected | | JIS K2536-2,4,5,6(1) |
| Methanol |  | Not detected | | JIS K2536-2,4,5,6(1) |
| Kerosene |  | Not detected | | JIS K2536-2,4(1) |
| (1) Other method that is traceable to national or international standard may be used. | | | | |

1. \* In accordance with the programme of work of the Inland Transport Committee for 2014–2018 (ECE/TRANS/240, para. 105 and ECE/TRANS/2014/26, programme activity 02.4), the World Forum will develop, harmonize and update Regulations in order to enhance the performance of vehicles. The present document is submitted in conformity with that mandate. [↑](#footnote-ref-2)
2. ECE/TRANS/WP.29/1045, as amended by Amends. 1 and 2 (Special Resolution No. 1, www.unece.org/trans/main/wp29/wp29wgs/wp29gen/wp29resolutions.html) [↑](#footnote-ref-3)