Proposal for the 03 series of amendments as Phase 3 of Regulation No. 129 (Enhanced Child Restraint Systems)

Submitted by the expert from France

The text reproduced below was prepared by the expert from France. It introduces the 03 series of amendments to Regulation No. 129 (Enhanced Child Restraint Systems (ECRS)) that were agreed upon by the experts of the Informal Working Group on Child Restraint Systems (IWG CRS). The modifications to the existing text of the UN Regulation in its 02 series of amendments, including:

* Proposal for supplement 1 to the 02 series of amendments - ECE/TRANS/WP.29/2017/63
* Proposal for supplement 2 to the 02 series of amendments - ECE/TRANS/WP.29/2017/126

are underlined and marked in bold for new or strikethrough for deleted characters. This document supersedes ECE/TRANS/WP.29/GRSP/2017/17 and GRSP-61-17-Rev.2. It includes all proposals of modifications made by the IWG ECRS during the two last meetings (2017/06/22&23 and 2017/08/31).

I. Proposal

*Paragraph 1*., amend to read:

"1. Scope

This Regulation applies (in Phases 1,**~~and~~** 2 **and 3**) to the following child restraint system for child occupants of power driven vehicles:

(a) Integral Universal ISOFIX Enhanced Child Restraint Systems (i-Size);

(b) Integral Specific vehicle ISOFIX Enhanced Child Restraint Systems;

(c) **~~n~~N**on-integral Universal Enhanced Child Restraint Systems (i-Size booster seat);

(d) **~~n~~N**on-integral **~~s~~S**pecific vehicle **~~e~~E**nhanced **~~c~~C**hild **~~r~~R**estraint **~~s~~S**ystems (**~~s~~S**pecific vehicle booster seat);

**(e) Integral Universal Belted Enhanced Child Restraint Systems;**

**(f) Integral Specific vehicle Belted Enhanced Child Restraint Systems."**

*Insert new paragraph 2.3*.*2.*, to read:

**"2.3.2. "*Universal Belted*" (Integral Universal Belted Enhanced Child Restraint System) is a category of Enhanced Child Restraint System primarily designed to be attached only by the adult safety seat belt in all Universal seating positions of a vehicle, as defined and approved according to Regulation No. 16."**

*Paragraph 2.3.2. (former)*, renumber as paragraph 2.3.3.

*Insert new paragraph 2.7.3.,* to read:

**"2.7.3. "*Specific vehicle Belted*" is a category of Integral Enhanced Child Restraint System connecting to specific vehicle types. All vehicle anchorages are to be approved according to Regulation No. 14 or [XX]. Additional attachment points required for securing rearward facing Enhanced Child Restraint System shall be checked according to Annex 25. It is also an indication for Enhanced Child Restraint Systems including dashboard as a vehicle contact zone."**

*Paragraph 2.12., amend to read:*

"2.12. "Anti-rotation device"

means a device intended to limit the rotation of the Enhanced Child Restraint System during a vehicle impact and consisting of:

(a) A top-tether strap; or

(b) A support-leg.

meeting the requirements of this Regulation and fitted to an ISOFIX anchorage system and ISOFIX top tether anchorages or vehicle floor contact surface meeting the requirements of Regulation No. 14 or Regulation No XX.

An "Anti-rotation device" for a "specific vehicle **~~ISOFIX~~**" Enhanced Child Restraint System may comprise a top tether, a support-leg or, **~~any other means capable of limiting the rotation~~ only for Rearward facing Enhanced Child Restraint System, a dashboard."**

*Paragraph 2.17.1.,* amend to read:

"2.17.1. "*ISOFIX Vehicle seat fixture*" means a fixture, according to ISOFIX size envelopes whose dimensions are given in Figures 1 to 7 of Appendix 2 to Annex 17 to Regulation No. 16, used by an Enhanced Child Restraint System manufacturer to determine the appropriate dimensions of **an Integral Universal Belted Enhanced Child Restraint System or** an ISOFIX Enhanced Child Restraint System **~~and~~ including** the location of its ISOFIX attachments."

Paragraph 2.26, amend to read :

**2.26. "Infant carrier"**

means an Integral Enhanced Child Restraint System restraining a child up to 15 months old and up to 87cm stature intended to accommodate the child in a rearward-facing semi-recumbent position. It is so designed as to distribute the restraining forces over the child's head and body excluding its limbs in the event of the frontal collision. It is designed to be removed from the vehicle with the child inside and without opening any harness and to carry it outside of the vehicle.

*Insert new paragraph 2.51.3.,* to read:

**"2.51.3. "*Universal seating position*" means a location in accordance with paragraph 8.2.2.5.2.(b) of Regulation No. 16."**

*Paragraphs 2.56.1. and 2.56.2.*, amend to read:

"2.56.1."*Class A device*" prevents the child from pulling the webbing of the retractor through to the lap part of the belt, when the adult belt is used to restrain the child directly **(Non-Integral Enhanced Child Restraint System).**

2.56.2."*Class B device*" **~~(to be used in phase III)~~** allows the retention of an applied tension in the lap part of an adult safety belt, when the adult belt is used to restrain **~~the~~ Integral** Enhanced Child Restraint System. The device intends to prevent the webbing from slipping from the retractor through the device, which would release the tension and place the restraint in a non-optimal position."

*Paragraph 2.57.,* amend to read:

"2.57. "*Module*", is a part of an **Enhanced Child Restraint System** that is separate from the ISOFIX attachments and is **hosting and restraining the child, ~~in direct contact with the child~~.** A module can be used **in combination with** **one or more** **~~a~~** **base ~~whether or~~**, **~~not~~ if allowed in this regulation,** or as a stand-alone **Integral ~~Universal~~ Belted** to restrain a child in a vehicle ~~car~~. **~~A base is allowed to accept more than one module (Module A, Module B, etc.).~~**"

*Insert new paragraph 2.58., to read:*

2.58. **“Base”, is a part of an Enhanced Child Restraint System that forms an interface between the vehicle and the module of an Enhanced Child Restraint System and has no direct contact with the child. A base is connected to the vehicle using ISOFIX anchorages or vehicle belt and an anti-rotation device if applicable.**

**A base is allowed to accept more than one module (Module A can be replaced by Module B, etc.).**

*Insert new paragraph 2.59., to read:*

**2.59. “Built in”, is an Enhanced Child Restraint System made as an integral part or incorporated as an add-on part of a vehicle. The vehicle manufacturer shall be the applicant for approval.**

*Insert new paragraph 2.60., to read:*

*2.60. “Belt route”, (global geometry of the belt)*


The belt route is the result of the combination of an ECRS to a specific seating position of the car.  There shall be only one belt route when a ECRS is installed to a specific seating position. If the belt route has an asymmetrical layout, it’s mirror images of the belt routing are defined as one belt routing.

When moving an ECRS from e.g. the left outboard seating position to the right outboard seating position the actual route of the adult vehicle belt can be different. If these actual routes differ only in symmetry, then these 2 actual routes are considered to be mirror images of the same belt route.

*Insert new paragraph 2.61., to read:*

*2.61. “Webbing path”, (points where the webbing has to pass)*

The webbing path is the path that an adult vehicle belt describes on a child restraint system. A typical non integral ECRS has a different webbing path when installed on the left outboard seating position compared to the webbing path used to install it in the right outboard seating position, as it uses not the left but the right shoulder belt guide.



*Paragraph 3.2.2.,* amend to read:

"3.2.2. The applicant shall indicate the kind of application:

(a) Application for an i-Size Enhanced Child Restraint Systems; or

(b) Application for a specific vehicle ISOFIX **Enhanced Child Restraint System**; or

(c) Application for a i-Size booster seat Enhanced Child Restraint System; or

(d) Application for a specific vehicle booster seat Enhanced Child Restraint System; **or**

**(e) Application for a Universal Belted Enhanced Child Restraint Systems; or**

**(f) Application for Specific vehicle Belted Enhanced Child Restraint Systems; or**

**(g)** Or any combination of (a),(b),(c) and (d)as long as they fulfil paragraph 5.4.2.2.**, 6.1.2.** and 6.1.3.**~~[3.]~~** **or**~~"~~

**(h) Any combination of (c), (d), (e), (f), as long as they fulfil paragraph 5.4.2.2. , 6.1.2. and 6.1.3.~~[3.]~~ provided there is only one belt route and that the booster seat is not equipped with ISOFIX connectors. "**

*Paragraph 4.3*., amend to read:

"4.3. The following information shall be clearly indicated on the product:

(a) The orientation of the Enhanced Child Restraint System relative to the vehicle;

(b) The size range(s) of the Enhanced Child Restraint System in centimetres;

(c) The maximum occupant mass allowed for the Integral Enhanced Child Restraint System in kilograms.

**~~If the Enhanced Child Restraint System is to be used in combination with an adult safety-belt, the correct webbing path shall be clearly indicated by means of a drawing permanently attached to the Enhanced Child Restraint System. If the restraint is held in place by the adult safety-belt, the webbing paths shall be clearly marked on the product by colour coding. The colours used for the path of the safety-belt when the device is installed in the forward-facing position shall be red and when installed in the rearward-facing shall be blue. The same colours shall also be used on the labels on the device that illustrate the methods of use.~~**

**~~There shall be a clear differentiation between the intended paths for the lap section and the diagonal section of the safety belt. Indication such as colour coding, words, shapes, etc. shall distinguish between sections of the safety belt.~~**

**~~The marking defined in this paragraph shall be visible with the Enhanced Child Restraint System in the vehicle, with the child in the Enhanced Child Restraint System~~."**

*Insert new paragraphs 4.6. to 4.6.3.*, to read:

**"4.6. Webbing path.**

**The markings defined in this paragraph shall be permanently and durably attached and visible with the Enhanced Child Restraint System installed in the vehicle, and with the child seated in the Restraint System. The markings shall be placed on both sides of the Enhanced Child Restraint System. The vehicle seat illustrated on the marking shall face the same direction as the real vehicle seat.**

**There shall be a clear differentiation between the intended paths for the lap section and the diagonal section of the safety belt. Indication such as colour coding, words, shapes, etc. shall distinguish between sections of the adult safety belt.**

**4.6.1. The adult safety belt route markings shall be placed on all belt guides and lock off devices. The adult safety belt route markings shall be at least the width of the adult belt path.**

**4.6.2. For Non-Integral Enhanced Child Restraint System to be used in combination with an adult safety-belt to restrain the child, the correct webbing path according to paragraph 6.1.3.4. shall be clearly marked on the product. This shall be by means of an installation drawing on a label permanently attached to the Enhanced Child Restraint System showing the correct path across the child’s body. The colour used for the adult belt route marking of the safety-belt when the device is installed shall be green. The same colour shall also be used for the belt path on the labels on the device that illustrate the installation.**

**4.6.3. For Integral Belted Enhanced Child Restraint System held in place by the adult safety-belt, the webbing paths according to paragraph 6.1.2.5. shall be clearly marked on the product, and indicated by means of a drawing permanently attached to the Enhanced Child Restraint System. The colour used for the path of the adult belt route marking, when the device is installed in the forward-facing or rearward-facing positions shall be green.same colour shall also be used on the labels on the device that illustrate the installation. "**

*Paragraphs 4.6. to 4.7.2.(former)*, renumber as paragraphs 4.7. to 4.8.2.

*Delete old Paragraph 4.7.3.*

**~~4.7.3. An impact shield that is not permanently attached to the child seat shall have a permanently attached label to indicate the make and model of the ECRS to which it belongs. The minimum size of the label shall be 40 x 40 mm.~~**

*Paragraph 4.8. (former), renumber as paragraph 4.12.*

*Insert new paragraphs 4.11. to 4.11.4.*, to read:

**"4.11. Marking for Integral Belted Enhanced Child Restraint System.**

**The marking shall be located on the part of the Enhanced Child Restraint System which includes the main load-bearing contact points.**

**One of the following information labels shall be permanently visible to the person installing the Enhanced Child Restraint System in a vehicle:**

**4.11.1. Universal Belted Enhanced Child Restraint Systems shall have a permanently attached label with the following information visible to the person installing the Enhanced Child Restraint System in the car:**

**Universal Belted **

**4.11.2. Specific vehicle Belted Enhanced Child Restraint System (including built-in systems) shall have a permanently attached label with the following information visible to the person installing the Enhanced Child Restraint System in the car:**

**Specific vehicle Belted **

**4.11.3. An international approval mark as defined in paragraph 5.4.1. In case the Enhanced Child Restraint System containing module(s) this marking shall be permanently attached to the part of the Enhanced Child Restraint System that includes the main load-bearing contact points.**


**4.11.4. An international module mark as defined in paragraph 5.4.3. In case the Enhanced Child Restraint System containing module(s) this marking shall be permanently attached to the module part of the Enhanced Child Restraint System."**

*New paragraph 4.12*., amend to read:

"4.12. Additional markings

"…

**(g) The shoulder beltpart and the lap belt part of the adult safety seat belt used for attaching infant carrier ~~Universal Belted or Specific vehicle Belted Enhanced Child Restraint Systems~~ shall be indicated with specific icons for shoulder belt path and lap belt path, visible for the user, close to the belt guiding area (icon A & B) or on the installation drawings (icon C). Icons A, B and C shall have the same colour coding [darker green on lap belt] as ~~like~~ used on the installation drawings and the minimum size is 20 mm in diameter.**



B

C

A

*Paragraph 5.4.2.1.,* amend to read:

"5.4.2.1. The words "i-Size universal ISOFIX", or "i-Size booster seat", or "specific vehicle ISOFIX" or "specific vehicle booster seat" **or "Universal Belted", or "Specific vehicle Belted",** depending on the category of Enhanced Child Restraint System;"

*Paragraph 5.4.3.1.,* amend to read:

"5.4.3.1. The words "R129" followed by a dash and the same approval number as the part of the **Enhanced Child Restraint System** which includes the ISOFIX attachments **or main load bearing contact points;"**

*Paragraph 6.1.2.2.,Table 1 amend to read:*

Table 1  
Possible configurations for type approval for Integral Enhanced Child Restraint Systems

|  | *Orientation* | *Category* | | | |
| --- | --- | --- | --- | --- | --- |
|  |  | i-Size ECRS | Integral Specific Vehicle ISOFIX ECRS | **Universal Belted** | **Specific vehicle Belted** |
| INTEGRAL | Lateral facing (Carry-cot) | NA | A | **NA** | **A** |
| Rearward facing | A | A | **A** | **A** |
| Forward facing | A | A | **A** | **A** |

*Note*:  
ECRS: Enhanced Child Restraint System  
A: Applicable  
NA: Non-Applicable

*Insert new paragraphs 6.1.2.3. to 6.1.2.6.*, to read:

**"6.1.2.3. For the "Universal Belted" category; this shall be by means of the adult safety seat belt only.**

**6.1.2.4. For the "Specific vehicle Belted" category; this shall be primarily by means of the adult safety seat belt.**

**6.1.2.5. Integral Enhanced Child Restraint Systems of the Belted categories shall have only one adult safety belt route and a main load-bearing contact point, between the Enhanced Child Restraint System and the adult safety belt on each side of the Enhanced Child Restraint System. This point shall not be less than 150 mm from the Cr axis when measured with the Enhanced Child Restraint System on the dynamic test bench installed in accordance with paragraph 7.1.3.5.2.3. of this Regulation, without a dummy. This shall apply to all adjustment setups and webbing paths.**

**6.1.2.6. The adult seat belt required to secure a Belted Integral Enhanced Child Restraint System on the dynamic test bench is defined in Annex 23 to this Regulation. The Enhanced Child Restraint System shall be secured onto the test bench using the appropriate standard seat belt described in Annex 23 using a preload tension of 50N ± 5N. The dummy shall not be installed unless the design of the restraint is such that the installation of a dummy would increase the length of belt used. With the Enhanced Child Restraint System in the installed position, there shall be no additional tension in the belt, apart from that exerted by the standard retractor (4 ± 3 N), where fitted. Where the retractor belt is used, this condition shall be met with at least 150 mm of belt remaining on the spool.**

**A clamping mechanism used according to paragraph 7.1.3.5.2.3. shall not influence the webbing path."**

*Paragraph 6.1.2.3.(former)*, renumber as paragraph 6.1.2.7.

*Paragraph 6.1.3.4.*, amend to read:

"6.1.3.4. Enhanced Child Restraint Systems of the **~~i-Size~~** booster seat categor**~~y~~ies** shall have **only one adult safety belt route and** a main load-bearing contact point, between the Enhanced Child Restraint System and the adult safety belt **on each side of the Enhanced Child Restraint System**. This point shall not be less than 150 mm from the Cr axis when measured with the Enhanced Child Restraint System on the dynamic test bench installed in accordance with paragraph 7.1.3.5.2.2. of this Regulation, without a dummy. This shall apply to all adjustment **~~configuration~~ setups and**  webbingpaths."

*Paragraph 6.2.1.5.*, amend to read:

“6.2.1.5. […] excessive stresses.

~~Moreover, the design shall be such that compression loads shall not be imposed on the crown of the child’s head in the event of a collision;~~

In the case of booster cushions and booster seats , the lap portion of the adult seat belt shall be positively guided on both sides to ensure that the loads are transmitted by the adult lap belt are transmitted through the pelvis. The positive guidance of loads over the pelvis shall be realised from the moment that the child is installed; the lap belt shall pass over the top of the thigh, just touching the fold with the pelvis. The angles α and β between the tangent line in which the belt touches the thighs and the horizontal shall be greater than 10°.

# Figures of Strapped child



*Paragraph 6.2.1.6*.*,* amend to read:

**"…**

**During the dynamic tests, the standard safety-belt used to install a non-integral Enhanced Child Restraint System, shall not become disengaged from any guide or locking device utilized for the test conducted; however, for the shoulder portion of the standard safety-belt this shall be judged up to the moment that the maximum horizontal head excursion of the dummy is reached."**

*Paragraph 6.2.1.10*.*,* amend to read:

"6.2.1.10. At least the worst case **~~configuration~~** of the dynamic test for the Enhanced Child Restraint System shall be performed after conditioning according to paragraph 7.2.6."

*Paragraph 6.2.3*., amend to read:

"6.2.3. It shall not be possible to remove or detach without the use of specific tools, any components not designed to be removable or detachable **for maintenance or change of configuration purpose**. Any components that are designed to be removable **or detachable ~~for maintenance or adjustment purpose~~** shall be so designed as to avoid any risk of incorrect assembly and use, as the assembly and disassembly processes shall be explained in detail in the restraint user guides. **For integral Enhanced Child Restraint Systems ~~A~~a**ny harness belt **or impact shield** shall be capable of its full range of adjustment without disassembly,"

*Paragraph 6.3.2.2.1*., amend to read:

"6.3.2.2.1. Integral Class Enhanced Child Restraint Systems

The maximum external dimensions for the width, height and depth of the Enhanced Child Restraint System and **if fitted,** the locations of the ISOFIX anchorages system, with which its attachments shall engage, shall be defined by the ISOFIX Vehicle Seat Fixture as defined in paragraph 2.17.1. of this Regulation.

(a) i-Size **or Universal Belted** Forward facing Enhanced Child Restraint Systems shall fit within the ISO/F2x size envelope for a reduced-height forward-facing toddler CRS;

(b) i-Size **or Universal Belted** Rearward facing Enhanced Child Restraint Systems shall fit within the ISO/R2 size envelope for a reduced-size rearward-facing toddler CRS;

(c) Specific vehicle ISOFIX **or Specific vehicle Belted** Enhanced Child Restraint Systems shall fit:

(i) in vehicle(s) specified in a list or

(ii) at least in one of the ISO (R1,R2X, R2, R3, F2X, F2, , F3, L1, L2) size envelopes as described in Annex 17 Appendix 2 of Regulation No. 16.

When conducting this assessment, the Integral Enhanced Child Restraint System shall be adjusted to the largest size of its declared stature range (height, depth and width dimensions as defined in Annex 18). If the Enhanced Child Restraint System is capable of being adjusted to different positions of seat surface inclination, the fitting assessment shall be done in at least one position. If other positions of inclination are outside the limits of the applicable size envelope, the user manual shall indicate that the child restraint may not fit in all approved vehicles when used in one of these positions.

**~~i-Size booster seats shall be adjusted to accommodate children of 135 cm stature (height, depth and width dimensions as defined in Annex 18) or to the largest size of its declared stature range in case the upper limit is below 135 cm. In this case, it must fit within each of its declared Vehicle Seat Fixtures in at least one adjustable position. The Enhanced Child Restraint System may be adjusted to other inclined positions (less or more reclined) that are outside the Vehicle Seat Fixture’s height; in this case, the child restraint manufacturer’s user manual shall clearly indicate that when used in one of these configuration arrangements, the Enhanced Child Restraint System may not fit in all vehicles approved for a Universal fixture.~~**

*Paragraph 6.3.2.2.2., amend to read:*

"6.3.2.2.2. Non-Integral Class Enhanced Child Restraint Systems

The maximum external dimensions for the width, height and depth of the Enhanced Child Restraint System and the locations of the ISOFIX anchorages system if any, with which its attachments shall engage, shall be defined by the i-Size booster seat fixture as defined in paragraph 2.17.2. of this Regulation.

(a) i-Size booster seat Enhanced Child Restraint Systems shall fit within the ISO/B2 size envelope;

(b) Specific vehicle booster seat Enhanced Child Restraint Systems shall fit:

(i) in vehicle(s) specified in a list; or

(ii) at least in one of ISO/B2 –ISO/B3 size envelope as described in Annex 17, Appendix 2 of regulation No. 16.

When conducting this assessment, the non-integral Enhanced Child Restraint System shall be adjusted to accommodate children of 135 cm stature (height, depth and width dimensions as defined in Annex 18) or to the largest size of its declared stature range if the upper limit is below 135 cm.

**~~If the Non-integral Enhanced Child Restraint System is capable of being adjusted to different positions of seat surface inclination, the fitting assessment shall be done in at least one position.~~**

**The Non-integral Enhanced Child Restraint System shall fit within the booster seat fixture in all angles of inclination of the fixture (90o-110o). The Enhanced Child Restraint System may be adjusted between inclination angles or positions to fit within the different booster seat fixture angles.**

If other positions of inclination are outside the limits of the applicable size envelope, the user manual shall indicate that the child restraint may not fit in all approved vehicles when used in one of these positions. If the Non-integral Enhanced Child Restraint System has a declared stature range above 135 cm, and if it is necessary to adjust the child restraint outside the limits of the applicable size envelope for such adjustments (height, depth and width dimensions), the user manual shall indicate that the child restraint may not fit in all approved vehicles when used in one of these positions.

*Paragraph 6.6.4.1.2., amend to read:*

"6.6.4.1.2. Enhanced Child Restraint Systems of the specific vehicle categories shall be assessed for fit with each vehicle model for which the Enhanced Child Restraint System is intended. The Technical Service responsible for conducting the test may reduce the number of vehicle **~~configurations~~ arrangements** tested if they do not differ greatly in the aspects listed in paragraph 6.6.4.1.2.3. of this Regulation. This Enhanced Child Restraint System shall be dynamically tested in one of the following ways: …"

*Paragraph 6.6.4.3.1., Table 5 amend to read:*

"…

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| Abdominal pressure**\*\*\*\*** | P | Bar | NA | NA | 1.2 | 1.0 | 1.0 | 1.2 |

\* HPC: see Annex 17.  
\*\* To be reviewed within 3 years following entry into force of the series 01 of this Regulation.  
\*\*\* Cum 3ms means cumulative 3ms value.

**\*\*\*\* Abdominal pressure, the highest recorded value is applicable for injury assessment (i.e, when the right handed sensors record 1.3 bar and the left handed sensor 1.0 bar, the recorded 1.3 bar is to be used for injury assessment)**"

*Paragraph 6.6.4.4.1.1.1., amend to read:*

“6.6.4.4.1.1.1. Where a test is conducted in accordance with paragraph**s** 6.6.4.1.6.**~~2~~1.1, 6.6.4.1.6.1.2**. **or paragraph 6.6.4.1.8.2.** above, a tolerance of +10 per cent shall be applicable to the head excursion value distance between Cr point and plane AB.”

*Paragraph 6.6.4.4.1.2.1, amend to read:*

6.6.4.4.1.2.1. Head excursion: no part of the head of the dummy shall pass beyond the planes FD, FG and DE, as shown in figure 2 below. This shall be judged up to 300 ms or the moment that the dummy has come to a definitive standstill whatever occurs first.

Except when testing using Q6 **or Q3** dummy where the value in relation to the FD plane is 840 mm

Where a test is conducted with paragraph**s** 6.6.4.1.6.**~~2~~1.1**. **or paragraph 6.6.4.1.6.1.2.** or paragraph 6.6.4.1.8.2. above, only the second **~~configuration~~** test results without 100 mm diameter bar will be considered.

Figure 2  
Arrangement for testing a rearward-facing device, not supported by the dashboard



"

*Insert new paragraphs 6.7.6. to 6.7.6.5.*, to read:

**"6.7.6. Lock-off device**

**6.7.6.1. The lock-off device shall be permanently attached to the Enhanced Child Restraint System.**

**6.7.6.2. The lock-off device shall not impair the durability of the adult belt and shall undergo the temperature test operation requirements given in paragraph 7.2.7.1.**

**6.7.6.3. The lock-off device shall not prevent the rapid release of the child.**

**6.7.6.4. Class A device**

**The amount of slip of the webbing shall not exceed 25 mm after the test prescribed in paragraph 7.2.9.1. below.**

**6.7.6.5. Class B device**

**The amount of slip of the webbing shall not exceed 25 mm after the test prescribed in paragraph 7.2.9.2. below."**

*Paragraph 7.1.2.7.,* amend to read:

"7.1.2.7. These tests shall be carried out using both the smallest and the largest appropriate dummy of the size range for which the restraining device is intended. Any adjustment of the dummy or Enhanced **~~child~~ Child ~~restraint~~ Restraint ~~systems~~ Systems** during the complete test cycle is not allowed."

*Paragraph 7.1.3*., amend to read:

"7.1.3. …

(e) The lateral dynamic test(s) will be performed in this(ese) **~~configuration~~ arrangement**(s);

…"

*Insert new paragraph 7.1.3.5.2.3., to read:*

**"7.1.3.5.2.3. Installation of an Integral Enhanced Child Restraint Systems "Universal Belted " seat or Specific vehicle Belted seat on the test bench.**

**The unoccupied belted Enhanced Child Restraint System shall be placed on the test bench.**

**Fit load cell 1 to the outboard position as shown Figure 1. Install the Enhanced Child Restraint System in the correct position. If a lock-off device is fitted to the Enhanced Child Restraint System and acts upon the diagonal belt, place load cell 2 at a convenient position behind the Enhanced Child Restraint System between the lock-off device and the buckle as shown above. If no lock-off device is fitted or if the lock-off device is fitted at the buckle, position the load cell at a convenient position between the pillar loop and the Enhanced Child Restraint System.**

**Adjust the lap portion of the reference belt to achieve a tension load of 50 N ± 5 N at load cell 1. Make a chalk mark on the webbing where it passes through the simulated buckle.**

**While maintaining the belt at this position, adjust the diagonal to achieve a tension of 50 N ± 5 N at load cell 2 by either locking the webbing at the Enhanced Child Restraint System webbing locker or by pulling the belt between the belt clamping mechanism and the standard retractor. If the tension in load cell 2 is achieved by pulling the belt between the clamping mechanism and the retractor, the clamping mechanism shall now be locked.**

**Extract all webbing from the retractor spool and rewind the excess webbing keeping a tension of 4 ± 3 N in the belt between the retractor and the pillar loop. The spool shall be locked before the dynamic test.**

**The dummy shall be placed in the Enhanced Child Restraint System separate from the seat-back of the chair by a flexible spacer. The spacer shall be 2.5 cm thick and 6 cm wide. It shall have length equal to the shoulder height less the thigh height, both in the sitting position and relevant to the dummy size being tested. The resulting height of the spacer is listed in the table below for the different dummy sizes. The board should follow as closely as possible the curvature of the seat and its lower end should be at the height of the dummy's hip joint.**

|  | ***Q0*** | ***Q1*** | ***Q1.5*** | ***Q3*** | ***Q6*** | ***Q10 (design targets)*** |
| --- | --- | --- | --- | --- | --- | --- |
|  | **Dimensions in mm** | | | | | |
| **Height of spacer device for positioning of dummy** | **173 ± 2** | **229 ± 2** | **237 ± 2** | **250 ± 2** | **270 ± 2** | **359 ± 2** |

**Adjust the Enhanced Child Restraint System belt in accordance with the manufacturer's instructions, but to a tension of 250 ± 25 N above the ~~adjuster~~ force needed to overcome the friction between the webbing and the adjuster, with a deflection angle of the strap at the adjuster of 45 ± 5°, or alternatively, the angle prescribed by the manufacturer.**

**The spacer shall then be removed and the dummy pushed towards to the seat back. Distribute the slack evenly throughout the harness.**"

*Paragraph 7.1.3.5.2.3.(former),* renumber as paragraph 7.1.3.5.2.4.

*Paragraph 7.1.3.6.2., amend to read:*

7.1.3.6.2. If the ~~i-Size~~ Enhanced Child Restraint System uses a top tether, one test shall be carried out with the smallest dummy with the shorter distance of the top tether (anchorage point G1). A second test shall be carried out with the heavier dummy with the longer distance of the top tether (anchorage point G2). Adjust the top tether to achieve a tension load of 50 ± 5 N. For side lateral impact the ISOFIX Enhanced child restraint shall be tested with only the shorter distance of the top tether.

*Paragraph 7.2.3.2., amend to read:*

"7.2.3.2.The free end of the strap shall be arranged in the same **~~configuration~~ way** as when the device is in use in the vehicle, and shall not be attached to any other part."

*Paragraph 7.2.5.2.6.2.,* amend to read:

"7.2.5.2.6.2. The table below sets out the general conditions for each test:

Table 8

|  | *Load (N)* | *Cycles per minute* | *Cycles (No.)* |
| --- | --- | --- | --- |
| Type 1 procedure | **~~10~~ Maximum 60** ± 0.**~~1~~5** | 30 ± 10 | 1 000 ± 5 |
| Type 2 procedure | **~~5~~ Minimum 10** ± 0.**~~05~~10** | 30 ± 10 | 5 000 ± 5 |

Where there is insufficient strap to test over 300 mm of shift, the test may be applied over a shorter length subject to a minimum of 100 mm.

*Paragraphs 7.2.5.2.6.3. to* 7.2.5.2.6.3.2.*,* amend to read:

"7.2.5.2.6.3. Particular test conditions

7.2.5.2.6.3.1. **~~Type 1 procedure: for cases where the strap slides through the quick adjusting device. The 10 N load shall be vertically and permanently applied on one of the straps. The other strap, set horizontally, shall be attached to a device, giving the webbing a back and forth motion. The adjusting device shall be so placed that the horizontal strap of the webbing remains under tension (see Annex 5, figure 1).~~**

**Type 1 procedure: for cases where the strap slides through the quick adjusting device. Apply a load of 10 N, if necessary the load may be increased by 10 N steps so as to permit correct sliding, but limited to a maximum of 60 N. This load shall be vertically and permanently applied on the straps. The part of the strap set horizontally shall pass through the quick adjuster it is fitted to and shall be attached to a device, giving the webbing a back and forth motion. The quick adjusting device shall be so placed that the horizontal strap of the webbing remains under tension (see Annex 5, Figure 1). Activate the quick adjuster while pulling the straps in the direction to slacken the harness and deactivate it while pulling the straps in the direction to tighten the harness.**

7.2.5.2.6.3.1. **~~Type 2 procedure: for cases where the strap changes direction in passing~~  ~~through a rigid part. During this test, the angles of both webbing straps~~  ~~shall be as shown in Annex 5, figure 2. The 5 N load shall be~~  ~~permanently applied. For cases where the strap changes direction more~~  ~~than once in passing through a rigid part, the load of 5 N may be~~  ~~increased so as to achieve the prescribed 300 mm of strap movement~~  ~~through that rigid part.~~**

**Type 2 procedure: for cases where the strap changes direction in passing through a rigid part. During this test, the webbing shall pass through the rigid part it is intended for and the test set up shall reproduce the angles as in the real installation (in three dimensions), see Annex 5, Figure 2 for examples. The 10 N load shall be permanently applied. For cases where the strap changes direction more than once in passing through a rigid part, the load of 10 N may be increased by 10 N steps so as to permit correct sliding and achieve the prescribed 300 mm of strap movement through that rigid part."**

*Insert new paragraphs 7.2.9. to 7.2.9.2.,* to read:

**"7.2.9. Lock-off devices**

**7.2.9.1. Class A devices**

**The Enhanced Child Restraint System and the largest manikin for which the Enhanced Child Restraint System is intended shall be set up as shown in Figure 4 below. The webbing used shall be as specifi ed in Annex 23 to this Regulation. The lock-off shall be fully applied and a mark made on the belt where the belt enters the lock-off. The force gauges shall be attached to the belt via a D ring, and a force equal to twice (±5 per cent) the mass of the heaviest dummy for the size range shall be applied for at least one second. The lower position shall be used for lock-offs in position A and the upper position for lock-offs in position B. The force shall be applied for a further 9 times. A further mark shall be made on the belt where it enters the lock-off and the distance between the two marks shall be measured. During this test, the retractor shall be unlocked.**

* **Figure 4**

**Retractor**

****

**Regulation No. 129**

**Test seat**

**15 kg manikin**

**Buckle/tongue**

**Examine for slippage**

**"D" ring**

**"Lock off" clip**

**Abdominal**

**Diagonal**

**Child seat**

**7.2.9.2. Class B devices.**

**The child restraint shall be firmly secured, and the webbing as specified in Annex 23 to this Regulation, shall be passed through the lock-off and frame following the routing described in the manufacturer's instructions. The belt shall pass through the testing equipment as described in Figure 5 below and be attached to a mass of 5.25 ± 0.05 kg. There shall be 650 ± 40 mm of free webbing between the mass and the point where the webbing leaves the frame. The lock-off shall be fully applied and a mark made on the belt where it enters the lock-off. The mass shall be raised and released so that it falls freely over a distance of 25 ± 1 mm. This shall be repeated 100 times ±2 at a frequency of 60 ± 2 cycles per minute, to simulate the jerking action of a child restraint in a car. A further mark shall be made on the belt where it enters the lock-off and the distance between the two marks shall be measured.**

**The lock-off device shall cover the full width of the webbing in the installed condition with Q3 dummy installed. This test is to be conducted using the same webbing angles as those formed in normal use. The free end of the lap belt portion shall be fixed. The test shall be conducted with the child restraint system firmly attached to the test bench used in the overturning or dynamic test. The loading strap can be attached to the simulated buckle."**

*Paragraph 8.1., amend to read:*

8.1. The test report shall record the results of all tests and measurements including the following test data:

(a) The type of device used for the test (acceleration or deceleration device),

(b) The total velocity change,

(c) The trolley speed immediately before impact only for deceleration sleds,

(d) The acceleration or deceleration curve during all the velocity change of the trolley and at least 300 ms,

(e) The time (in ms) when the head of the manikin reaches its maximum displacement during the performance of the dynamic test,

(f) The place occupied by the buckle during the tests, if it can be varied, and

(g) The name and address of the laboratory where tests have been performed,

(h) And any failure or breakage,

(i) The following dummy criteria: HPC, Head acceleration Cum3ms, Upper neck tension force, Upper neck moment, Chest acceleration

Cum3ms, Chest deflection; Abdominal Pressure (in frontal **and rear** impact); and

(j) Adult Seat belt bench installation forces.

*Paragraph 9.2.1.1., amend to read:*

"9.2.1.1. Five Enhanced Child Restraint Systems shall be subjected to the dynamic test described in paragraph 7.1.3. above. The Technical Service that conducted the type approval tests shall choose the conditions that produced the maximum horizontal head excursion during the type approval dynamic tests, excluding the conditions described in paragraph**s** 6.6.4.1.6.**~~2~~1.1**., **6.6.4.1.6.1.2.** and paragraph 6.6.4.1.8.2. above. All the five Enhanced Child Restraint Systems shall be tested under the same conditions."

*Insert new paragraph 14.2.3.,* to read:

**"14.2.3. For Universal Belted seat category Enhanced Child Restraint Systems the following label shall be clearly visible on the exterior of the packing:**

| ***Notice:* This is an Universal Belted Enhanced Child Restraint System. It is approved according to Regulation No.129, for use primarily in "Universal seating positions" as indicated by vehicle manufacturers in the vehicle users’ manual.**  **If in doubt, consult either the Enhanced Child Restraint System manufacturer or the retailer*.*** |
| --- |

*"*

*Paragraphs 14.2.3. to 14.2.9. (former),* renumber as paragraphs 14.2.4. to 14.2.10.

*Insert new paragraphs 16.8. to 16.10.,* to read:

**"16.8. As from the official date of entry into force of the 03 series of amendments to this Regulation, no Contracting Party applying this Regulation shall refuse to grant or refuse to accept type approvals to this Regulation as amended by the 03 series of amendments.**

**16.9. Until 1 September 2020, type approvals to the preceding series of amendments to the Regulation which are not affected by the 03 series of amendments to the Regulation shall remain valid and Contracting Parties applying this Regulation shall continue to accept them.**

**16.10. Until 1 September 2022, Contracting Parties applying this Regulation shall not refuse to grant extensions of approval to the 01 and 02 series of amendments to this Regulation."**


*Annex 2, replace current Annex 2 by the following to read:*

"Annex 2

# **1. Arrangements of the approval mark**


**Replace all 02 by 03**

… according to which the approval has been granted.

****

**In the figure replace i-Size universal ISOFIX by Universal Belted, delete the mass limit and replace 02 by 03**

**The Enhanced Child Restraint System bearing the above approval mark is a device capable of being fitted in any universal seating position of the vehicle and of being used for the 40 cm - 70 cm size range; it is approved in France (E 2) under the number 032439. The approval number indicates that the approval was granted in accordance with the requirements of the Regulation concerning the approval of Universal Belted Enhanced Child Restraint Systems used on-board of motor vehicles as amended by the 03 series of amendments. In addition the name of the regulation has to be identified on the approval mark followed by the series of amendment according to which the approval has been granted.**


****

**In the figure replace ISOFIX by Belted, delete the mass limit and replace 02 by 03**


**The Enhanced Child Restraint System bearing the above approval mark is a device not capable of being fitted in every vehicle and capable of being used for the 40 cm - 70 cm size range; it is approved in France (E 2) under the number 032450. The approval number indicates that the approval was granted in accordance with the requirements of the Regulation concerning the approval of Specific vehicle Belted Enhanced Child Restraint Systems used on-board of motor vehicles as amended by the 03 series of amendments. In addition the name of the regulation has to be identified on the approval mark followed by the series of amendment according to which the approval has been granted.**

In case the E**nhanced** C**hild** R**estraint** S**ystem** is equipped with a module, the size range **and the mass limit are** **~~is~~** not on the approval mark but on the module mark.

# **2. Arrangements of the approval mark in combination with a module mark**

**Insert 03**

The Enhanced Child Restraint System bearing the above approval mark is a device, including module(s), capable of being fitted in any i-size compatible vehicle seating position. It is approved in France (E 2) under the number 0**~~2~~3**2439. The approval number indicates that the approval was granted in accordance with the requirements of the Regulation concerning the approval of Enhanced Child Restraint Systems used on-board of motor vehicles as amended by the 0**~~2~~3** series of amendments. In addition the name of the regulation has to be identified on the approval mark followed by the series of amendment according to which the approval has been granted.


**Insert 03**

The Enhanced Child Restraint System bearing the above approval mark is a device, including module(s), not capable of being fitted in every vehicle. It is approved in France (E 2) under the number 0**~~2~~3**2450. The approval number indicates that the approval was granted in accordance with the requirements of the Regulation concerning the approval of Specific vehicle ISOFIX Enhanced Child Restraint Systems used on-board of motor vehicles as amended by the 0**~~2~~3** series of amendments. In addition the name of the regulation has to be identified on the approval mark followed by the series of amendment according to which the approval has been granted.

## **2.1. Arrangements of the module mark in combination with an approval mark**

**2.1.1. Where a module is approved for use with more than one base, the individual base and module combinations shall be indicated on the module in separate module marks, each bearing their applicable size ranges.**



**~~An Enhanced Child Restraint System~~ A Module that bears an approval mark for the stand-alone mode of use and a module mark for its use on three different bases, shall carry the following arrangement of approval and module marks:**

**Replace in the first figure Infant Carrier Module "name of the module" by "Universal Belted"**

**The ~~Enhanced Child Restraint System~~ modulebearing the above marks is capable of being used as an Universal Belted Enhanced Child Restraint System ~~Infant Carrier~~ ~~Module with a vehicle belt]~~ for the 45 cm - 75 cm size range; it is approved according to regulation No. 129-03 under the number 032348.**

**The ~~Enhanced Child Restraint System~~ module can also be used as a module in combination with the base "brand name & model A’, for the 45 cm - 75 cm size range and mass limit of 12 kg; approved according to Regulation No. 129-03 under the number 032439.**

**The ~~Enhanced Child Restraint System~~ module can also be used as a module in combination with the base "brand name & model B’, for the 45 cm - 75 cm size range and mass limit of 12 kg; approved according to Regulation No. 129-03 under the number 032440.**

**The ~~Enhanced Child Restraint System~~ module can also be used as a module in combination with the base "brand name and model C", for the 45 cm - 75 cm size range and mass limit of 12 kg; approved according to Regulation No. 129-03 under the number 032441.**

**The approval numbers indicate that the approval was granted in accordance with the requirements of the Regulation concerning the approval of Enhanced Child Restraint Systems used on board of motor vehicles as amended by the 03 series of amendments.**

**2.1.2. Where a module is capable of being installed in different orientations, separate module marks shall be indicated on the module, each bearing their applicable size ranges.**

****

**The ~~Enhanced Child Restraint System~~ module bearing the above marks is capable of being used in a rearward facing mode with the base "brand name & model A’, for the 60 cm - 105 cm size range and with a mass limit of 18 kg; approved according to Regulation No. 129-03 under the number 032441.**

**The ~~Enhanced Child Restraint System~~ module bearing the above marks is also capable of being used in a forward facing mode with the base "brand name and model A", for the 85 cm - 105 cm size range and with a mass limit of 18 kg; approved according to Regulation No. 129-03 under the same number 032441.**

**The approval number indicates that the approval was granted in accordance with the requirements of the Regulation concerning the approval of Enhanced Child Restraint Systems used on-board motor vehicles as amended by the 03 series of amendments.**

**2.2 Examples of the symbols to be used on the module mark are given in the figures below. As chosen by the Enhanced Child Restraint Systems manufacturer, one of the symbols or an equivalent shall be used on the module mark. ”**

****

*Annex 5, Figures 1 and 2* , amend to read:

"Annex 5

Abrasion and microslip test

Figure 1

**Procedure type 1**

F = 10 ± 0.1 N**, can be increased up to maximum F = 60 ± 0.5 N (e.g. table 8 §7.2.5.2.6.2)**

Total travel:

300 ± 20 mm

Support

Protective strap for inner bar

Example a

Example b

Examples of test arrangements corresponding

to the type of adjusting device

F = 10 ± 0.1 N**, can be increased up to maximum F = 60 ± 0.5 N (e.g. table 8 §**7.2.5.2.6.2)

Total travel:

300 ± 20 mm

Lower stop

Rotating pin

Figure 2

**Procedure type 2**

**Following two examples of test set up**

**Example 1**

Straps in horizontal plane

**Minimum F = 10 ± 0.1 N** **~~F = 5 ± 0.05 N~~ (e.g. table 8 §7.2.5.2.6.2)**

**α**

**±**

**5°**

Total travel:

300 ± 20 mm

Test in the buckle

**Example 2**

**α**

**±**

**5º**

**β**

**±**

**5º**

**Minimum F = 10 ± 0.1 N F ~~= 5 ±0.05 N~~ (e.g. table 8 §7.2.5.2.6.2)**

Total travel:

300 ± 20 mm


Test in a guide or pulley

**Where α and β reproduce the angles as in the real installation (in three dimensions)**

..."

*Annex 6, appendix 2, insert new figure 5:*

**Figure 5: Lower strap anchorages (LSA 1, LSA 2, LSA 3 and LSA 4)**

**New**

*Annex 8, Note Table 1, amend to read:*

The installation of Abdominal Pressure Twin Sensors (APTS) in frontal **and rear** impact may add up 0.2 kg to the Q1.5 and 0.5kg to the Q3, Q6 and Q10 dummies.

*Annex 8, Table 2*, amend to read:

Table 2

**Q-dummy dimensions**

| *No.* |  | *Q0* | *Q1* | *Q1.5* | *Q3* | *Q6* | *Q10 (design targets)* |
| --- | --- | --- | --- | --- | --- | --- | --- |
|  |  | *Dimensions in mm* | | | | | |
| 17 | Seating height  (head tilted forward) | 355 ± 9 | 479 ± 9 | 499 ± 9 | 544 ± 9 | 601 ± 9 | **~~< 748 ± 9~~**  **733.7 ± 9** |
| 18 | Shoulder height  (sitting) | **~~225 ± 7~~**  **255 ± 5** | 298 ± 7 | 309 ± 7 | 329 ± 7 | 362 ± 7 | 473 ± 7 |
|  | Stature (head tilted forward) | - | 740 ± 9 | 800 ± 9 | 985 ± 9 | 1143 ± 9 | **~~< 1443 ± 9~~**  **1453.2 ± 12** |
| 5 | Chest depth | - | 114 ± 5 | 113 ± 5 | 146 ± 5 | 141 ± 5 | 171 ± 5 |
| 15 | Shoulder width | **~~230 ± 7~~**  **145 ± 5** | 227 ± 7 | 227 ± 7 | 259 ± 7 | 305 ± 7 | 334.8 ± 7 |
| 12 | Hip width | - | 191 ± 7 | 194 ± 7 | 200 ± 7 | 223 ± 7 | 270 ± 7 |
| 1 | Back of buttocks to front of knees | 130 ± 5 | 211 ± 5 | 235 ± 5 | 305 ± 5 | 366 ± 5 | 485.4 **~~± 5~~± 6** |
| 2 | Back of buttocks to popliteus | - | 161 ± 5 | 185 ± 5 | 253 ± 5 | 299 ± 5 | 414,9 **~~± 5~~± 6** |
| 21 | Thigh height, sitting |  | 69 | 72 | 79 | 92 | 114 **± 3** |
|  | Height of spacer device for positioning of dummy1 |  | 229 ± 2 | 237 ± 2 | 250 ± 2 | 270 ± 2 | 359 ± 2 |

*Annex 12, paragraph 2.2.1.4., Notes*, amend to read:

"*Notes*:  
MH means harder ~~configuration~~ condition (the least good results obtained in approval or extension of approval)  
LH signifies a less hard ~~configuration~~ condition."

*Annex 18*, amend to read:

"Annex 18

Geometrical dimensions of Enhanced Child Restraint Systems

Figure 3 **Side and Front View of the measuring device for measurements applicable to Enhanced Child Restraint Systems that feature an impact shield**

|  |  |
| --- | --- |
|  |  |

**New** 

All dimensions in mm

Internal geometry assessment method

*Replace in the entire paragraph ECRS by Enhanced Child Restraint System*

*Annex 18, insert new paragraph 3*

**3. Stature Calculation**

**The measurements taken in Section 1 & 2 shall then be compared to the values shown in Annex 18, Table 1.**

**Interpolation between the values shown in the table is allowed in one-centimetre intervals**

**For each measurement, the corresponding stature at the nearest whole lower centimetre shall be calculated.**

**Maximum stature**

**For the measurements B, C, D, E2, F2 and G2 the measured value must be greater or equal to the value shown in the table to meet the stature requirement.**

**e.g. To declare a stature of 105 cm the measured sitting hight after applying tolerances must be greater or equal to 61.8 cm**

**The maximum stature is the smallest stature calculated from the measurements B, C, D, E2, F2 and G2.**

**Minimum stature**

**For the measurements E1, F1 and G1 the measured value must be less than or equal to the value shown in the table to meet the stature requirement.**

**e.g. To declare a stature of 100 cm the measured shoulder height after applying tolerances must be less than or equal to 32.4 cm**

**The minimum stature is the largest stature calculated from the measurements E1, F1 and G1."**

*Annex 20, replace ECRS by Enhanced Child Restraint System*

*Annex 22, to be deleted.*

*Annex 23, amend to read:*

"1. The safety-belt for the dynamic test and for the maximum length requirements shall be made according to the ~~configuration~~ definition shown in Figure 1. These are a three-point retracting belt system.

…"

*Insert new Annex 25,*

**"Annex 25**

**Additional attachment points required for securing rearward facing Enhanced Child Restraint System, of category Specific vehicle Belted, to motor vehicles**

**1. This annex applies only to the additional anchorages for attaching Enhanced Child Restraint in the Specific vehicle Belted category or to bars or other special items used to secure child-restraining devices to the bodywork, whether or not they make use of the Regulation No. 14 or [xx] anchorages.**

**2. The anchorages shall be determined by the manufacturer of the child restraint system and details shall be submitted for approval to the Technical Service conducting the tests.**

**The Technical Services may consider information obtained from the vehicle manufacturer.**

**3. The manufacturer of the child restraint shall provide the necessary parts for fitting the anchorages. and a special plan for each vehicle showing their exact location.**

**4. The child restraint manufacturer shall indicate if the anchorages required for attaching the restraint to the car structure are in accordance with the position and strength requirements of paragraph 3. onwards in the recommendation given to Governments intending to adopt specific requirements relating to anchorages for child restraints used in passenger cars.**

II. Justification

1. The proposed amendment includes Enhanced Child Restraint Systems from the universal Belted or specific to vehicle Belted categories into the scope of UN Regulation No. 129. This represents Phase 3 of the UN Regulation.

2. The text includes all modifications proposed by GRSP up to and including its sixty-first (8-12 May 2017) as well as those of the Informal Working Group on Child Restraint Systems up to and including its sixty-seventh session (Brussels, 31th August 2017).

3. This proposal refers to the series 02 text of Regulation No. 129, including the following amendments:

* Proposal for supplement 1 to the 02 series of amendments - ECE/TRANS/WP.29/2017/63
* Proposal for supplement 2 to the 02 series of amendments - ECE/TRANS/WP.29/2017/126