**Photometric compliance and testing requirements**

**SLR-28-12**

“status quo” R-LSD + R-RID

|  |  |
| --- | --- |
|  | Photometric compliance requirement (X=yes) |
|  |  | 200ms | 4s | 1min | 10min | 30minstability | >>100h (Light-Source level) |
| StopDI |  |  |  | XLED |  | Xall | XNon-replaceable filament L-S IEC 60809 / 60810 (light-source level)Replaceable L-S all |
| DI sequential |  | Xall |  | XLED |  | Xall |
| PositionSide-markerRear-fog |  |  |  | XLED |  | Xall |
| DRL |  |  |  | XLED |  | Xall |
| ConeringReversingManouvering |  |  |  | XLED | Xall |  |
| Low beam, AFSFront-Fog |  |  | (X)HID | XLED |  | X all |
| High beam, ADB |  |  | (X)HID | XLED |  | X all |
|  |  |  |  |  |  |  |  |

Testing requirement

all

filament

LED

HID

Other

„future“ R-LSD + R-RID

|  |  |
| --- | --- |
|  | Beam-compliance requirement (X=yes for all) |
|  |  | 200ms | 4s | 1min | 10min | 30minstability | >>100h (Light-Source level) |
| StopDI |  | XHIDother | X | XLEDHIDother | X | Xall | XNon-replaceable L-S / modulesReplaceable L-S |
| DI sequential |  | Xall | XHIDother | XLEDHIDother | X | Xall |
| PositionSide-markerRear-fog |  | n/a | XHIDother | XLEDHIDother | X | Xall |
| DRL |  | n/a | XHIDother | XLEDHIDother | X | Xall |
| CorneringReversingManouvering |  | n/a | XHIDother | XLEDHIDother | Xall | n/a |
| Low beam, AFSFront-Fog |  | n/a | XHIDother | XLEDHIDother | X | X all |
| High beam, ADB |  | n/a | XHIDother | XLEDHIDother | X | X all |
|  |  |  |  |  |  |  |  |