**BMFE 08-XX**

**I Proposal**

*UN R 118, No. 5, Part I, insert new paragraph 5.2.5. and 5.2.6. to read:*

“5.2.5. Single materials fulfilling the relevant requirements of 6.2.1.-6.2.7., that are bonded together by an adhesive agent not exacerbating the burning behaviour are considered to fulfil the requirements as a composite material.

5.2.6. If an adhesive agent, that is not declared to not deteriorate the burning behaviour of the interior material is used to affix the interior material to its supporting structure, such material shall be tested in combination with the adhesive agent and a possible supporting structure.”

UN R118, Annex 1 – Information document for vehicle

*Insert new paragraph 4. and 4.1. to read:*

“4. Adhesive agents

4.1. In cases where adhesive agents are used to affix the material to supporting structures or bonding materials together to a composite material and these material is not tested or approved by a component type approval, a list of adhesive agents that can be used without deterioration of the burning behaviour of the material(s): ……. “

UN R118, Annex 2 - Information document for component

*Insert new item 5. and 5.1. to read:*

“5. Adhesive agents

5.1. In cases where adhesive agents are used to affix the material to supporting structures or bonding materials together to a composite material, a list of adhesive agents that can be used without deterioration of the burning behaviour of the material(s): …….“

**II Justification**