**SLR-45-17/Rev.1**

*(based on of SLR-44-16/Rev.1)*

**Proposal for a Supplement to the 01 series of Regulation No. 86 (Installation of lighting and light-signalling devices for agricultural vehicles)**

 **Submitted by the Informal Working Group on Simplification of Lighting and Light-Signalling Regulations (IWG SLR)**

The text reproduced below was prepared by IWG SLR with the aim to introduce into the 01 series of amendments to Regulation No. 86 references to the headlamp Classes in the 01 series of amendments to UN Regulation No. 149. The modifications to the existing text of Regulation No. 86 are marked in bold for new or strikethrough for deleted characters

 I. Proposal

*Paragraph 6.1.2.,* amend to read:

"6.1.2. Number: Two ~~or four~~**, type‑approved according to:**

 **- UN Regulations Nos. 98 or 112 or 113,**

**or**

**- Classes A, B, BS, CS, D, DS or ES of the 00 series of amendments to UN Regulation No. 149,**

**or**

**- Classes A, B, BS, CS or DS of the 01 and subsequent series of amendments to UN Regulation No. 149.**

**Optionally one additional pair type‑approved according to:**

**- UN Regulations Nos. 98 or 112 or 113,**

**or**

**- Classes A, B, BS, CS, D, DS or ES of the 00 series of amendments to UN Regulation No. 149,**

**or**

**- Classes A, B, BS, CS, DS or RA of the 01 and susbsequent series of amendments to UN Regulation No. 149.**"

*Paragraph 6.1.9.2.,* amend to read:

"6.1.9.2. This maximum intensity shall be obtained by adding together the individual reference marks which are indicated on the several headlamps. ~~The reference mark "10" shall be given to each of the headlamps marked "R" or "CR".~~"

*Paragraph 6.2.2.,* amend to read:

"6.2.2. Number: Two (or four - see paragraph [6.2.4.2.4.](http://srace2:8080/document/show/document_id/1771#A0_S6_2_3_2_1_))**, type‑approved according to:**

 **- UN Regulations Nos. 98 or 112 or 113,**

**or**

 **- Classes A, AS, B, BS, CS, D, DS or ES of the 00 series of amendments to UN Regulation No. 149,**

**or**

 **- Classes AS, BS, C, CS, DS or V of the 01 and subsequent series of amendments to UN Regulation No. 149.**"

 II. Justification

With the entry into force of the new series of amendments (01) to UN Regulation No. 149 produced by IWG SLR, it is necessary to introduce alternative references to Regulation No. 86. This amendment deals with such additional references for the 01 series amendments to UN Regulation No 86

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_