2.2 *"Vehicle type with regard to its Direct Vision"* means vehicles which do not differ in such essential respects as:

(a) The manufacturer's trade name or mark;

(b) The dimensions and shapes of the components of the vehicle structure situated in front of a vertical plane positioned 1000mm behind the driver’s eye point (E2) and perpendicular to the longitudinal plane of the vehicle;

(c) The distance in the X axis between the Accelerator Heel Point and the foremost point of the vehicle;

(d) The number, size, shape or location of transparent areas of the vehicle situated in front of a vertical plane positioned 1,000 mm behind the driver’s eye point (E2) and perpendicular to the longitudinal plane of the vehicle;

(e) The direct vision level, as defined by the table in Annex 5, that the vehicle will fall into.